{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":14,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHSCU-CL3"]
[]
[]
[]
[]
["","","","","","JEHSCU0300CL3","JEHSCU0400CL3","JEHSCU0500CL3","JEHSCU0600CL3","JEHSCU0750CL3","JEHSCU0951CL3 EVI","JEHSCU0951CL3 EVI_","JEHSCU0200CL3 (Archived)","JEHSCU0950CL3 EVI (Archived)"]
["Kylkapacitet","Low temperature","R-407F","Nom","kW","","2.38","2.87","","","","","","4.88"]
["Årlig elförbrukning Q","R-407F","","Te -35°C","kWh/a","","10,730.00","13,018.00","","","","","","22,348.00"]
["Parameters at full load and ambient temp. 43°C","R-407F","Te -35°C","Power input (D3)","kW","","3.30"]
["","","","Kylkapacitet (P3)","kW","","2.04"]
["","","","Deklarerad COP (COP3)","","","0.62"]
["Vikt","Enhet","","","kg","78","132","132","133","203","","","76","200"]
["Köldmedium","GWP","","","","","","","","","","","3,922"]
["","Typ","","","","","","","","","","","R-404A"]
["Prestandaförhållande på årstidsrelaterad verkningsgrad SEPR","R-407F","","Te -35°C","","","1.65","1.64","","","","","","1.63"]
["Parametrar vid fullast och omgivningstemp. 32°C (punkt A)","R-407F","Te -35°C","Märkt ineffekt (DA)","kW","","2.51","3.08","","","","","","4.51"]
["","","","Märkt COP (COPA)","","","0.95","0.93","","","","","","1.08"]
["","","","Märkt kylkapacitet (PA)","kW","","2.38","2.87","","","","","","4.88"]
["COP","Låg temperatur","","R-407F","","","0.95","0.93","","","","","","1.08"]
["Mått","Enhet","","Bredd","mm","1,101","1,353","1,353","1,353","1,348","","","1,101","1,348"]
["","","","Djup","mm","444","575","575","575","605","","","444","605"]
["","","","Höjd","mm","662","872","872","872","1,727","","","662","1,727"]
["Hölje","Färg","","","","Ljusgrå","Ljusgrå","Ljusgrå","Ljusgrå","Ljusgrå","","","Ljusgrå","Ljusgrå"]
["Fläkt","Typ","","","","Axiell","Axiell","Axiell","Axiell","Axiell","","","Axiell","Axiell"]
["Power supply","Fas","","","","3~","3~","3~","3~","3~","","","3~","3~"]
["","Frequency","","","Hz","50","50","50","50","50","","","50","50"]
["","Spänning","","","V","400","400","400","400","400","","","400","400"]
["Anm:","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - Se villkor: Utomhustemperatur = 32°C, avdunstningstemperatur = -10°C och 10K superheat (medium temperaturapplikation)"]
["","","","","","(2) - Ljudtrycksnivån är uppmätt vid 10 m i ett ekofritt rum.","(2) - Ljudtrycksnivån är uppmätt vid 10 m i ett ekofritt rum.","(2) - Ljudtrycksnivån är uppmätt vid 10 m i ett ekofritt rum.","(2) - Ljudtrycksnivån är uppmätt vid 10 m i ett ekofritt rum.","(2) - Ljudtrycksnivån är uppmätt vid 10 m i ett ekofritt rum.","","","(2) - Ljudtrycksnivån är uppmätt vid 10 m i ett ekofritt rum.","(2) - Ljudtrycksnivån är uppmätt vid 10 m i ett ekofritt rum."]
["","","","","","(3) - Dess funktion är avhängigt fluorerande växthusgas","(3) - Dess funktion är avhängigt fluorerande växthusgas","(3) - Dess funktion är avhängigt fluorerande växthusgas","(3) - Dess funktion är avhängigt fluorerande växthusgas","(3) - Dess funktion är avhängigt fluorerande växthusgas","","","(3) - Dess funktion är avhängigt fluorerande växthusgas","(3) - Dess funktion är avhängigt fluorerande växthusgas"]
["Kylkapacitet","Låg temperatur","R-407A","Nom","kW","","","","","","4.89","4.89"]
["","","R-407F","Nom","kW","","","","","","4.90","4.90"]
["","","R-448A","Nom","kW","","","","","","4.85","4.85"]
["","","R-449A","Nom","kW","","","","","","4.85","4.85"]
["Ineffekt","Låg temperatur","R-407A","Nom","kW","","","","","","4.15","4.15"]
["Effektförbrukning","Låg temperatur","R-407F","Nom","kW","","","","","","3.86","3.86"]
["Ineffekt","Låg temperatur","R-448A","Nom","kW","","","","","","3.95","3.95"]
["","","R-449A","Nom","kW","","","","","","3.95","3.95"]
["COP","Låg temperatur","","R-407A","","","","","","","1.18","1.18"]
["","","","R-407F","","","","","","","1.27","1.27"]
["","","","R-448A","","","","","","","1.23","1.23"]
["","","","R-449A","","","","","","","1.23","1.23"]
["Årlig elförbrukning Q","R-407A","","Te -35°C","kWh/a","","","","","","22108.00","22108.00"]
["","R-407F","","Te -35°C","kWh/a","","","","","","20961.00","20961.00"]
["","R-448A","","Te -35°C","kWh/a","","","","","","21477.00","21477.00"]
["","R-449A","","Te -35°C","kWh/a","","","","","","21477.00","21477.00"]
["Prestandaförhållande på årstidsrelaterad verkningsgrad SEPR","R-407A","","Te -35°C","","","","","","","1.65","1.65"]
["","R-407F","","Te -35°C","","","","","","","1.74","1.74"]
["","R-448A","","Te -35°C","","","","","","","1.68","1.68"]
["","R-449A","","Te -35°C","","","","","","","1.68","1.68"]
["Parametrar vid fullast och omgivningstemp. 32°C (punkt A)","R-407A","Te -35°C","Märkt kylkapacitet (PA)","kW","","","","","","4.89","4.89"]
["","","","Märkt ineffekt (DA)","kW","","","","","","3.15","3.15"]
["","","","Märkt COP (COPA)","","","","","","","1.18","1.18"]
["","R-407F","Te -35°C","Märkt kylkapacitet (PA)","kW","","","","","","4.90","4.90"]
["","","","Märkt ineffekt (DA)","kW","","","","","","3.86","3.86"]
["","","","Märkt COP (COPA)","","","","","","","1.27","1.27"]
["","R-448A","Te -35°C","Märkt kylkapacitet (PA)","kW","","","","","","4.85","4.85"]
["","","","Märkt ineffekt (DA)","kW","","","","","","3.95","3.95"]
["","","","Klassad COP (COPA)","","","","","","","1.23","1.23"]
["","R-449A","Te -35°C","Märkt kylkapacitet (PA)","kW","","","","","","4.85","4.85"]
["","","","Märkt ineffekt (DA)","kW","","","","","","3.95","3.95"]
["","","","Klassad COP (COPA)","","","","","","","1.23","1.23"]
["Hölje","Färg","","","","","","","","","Ljusgrå","Ljusgrå"]
["Mått","Enhet","","Höjd","mm","","","","","","1727","1727"]
["","","","Bredd","mm","","","","","","1348","1348"]
["","","","Djup","mm","","","","","","605","605"]
["Vikt","Enhet","","","kg","","","","","","200","200"]
["Fläkt","Typ","","","","","","","","","Axiell","Axiell"]
["Köldmedium","Typ 2","","","","","","","","","R-407A","R-407A"]
["","Typ 3","","","","","","","","","R-407F","R-407F"]
["","Typ 5","","","","","","","","","R-448A","R-448A"]
["","GWP Typ 2","","","","","","","","","2107","2107"]
["","GWP Typ 3","","","","","","","","","1825","1825"]
["","GWP Typ 5","","","","","","","","","1387","1387"]
["Strömförsörjning","Fas","","","","","","","","","3~","3~"]
["","Frequency","","","Hz","","","","","","50","50"]
["","Spänning","","","V","","","","","","400","400"]
["Enhet","Nominell driftström (RLA)","R-448A","Kyla","A","","","","","","8.50","8.50"]
["","","R-449A","Kyla","A","","","","","","8.50","8.50"]
["Anm:","","","","","","","","","","(2) - Ljudtrycksnivån är uppmätt vid 10 m i ett ekofritt rum.","(2) - Ljudtrycksnivån är uppmätt vid 10 m i ett ekofritt rum."]
["Årlig elförbrukning Q","R-404A","","Te -35°C","kWh/a","","","","","","","24503"]
["Prestandaförhållande på årstidsrelaterad verkningsgrad SEPR","R-404A","","Te -35°C","","","","","","","","1.79"]
["Parametrar vid fullast och omgivningstemp. 32°C (punkt A)","R-404A","Te -35°C","Märkt kylkapacitet (PA)","kW","","","","","","","5.90"]
["","","","Märkt ineffekt (DA)","kW","","","","","","","4.35"]
["","","","Märkt COP (COPA)","","","","","","","","1.36"]
["Parametrar vid fullast och omgivningstemp. 43°C","R-404A","Te -35°C","Deklarerad COP (COP3)","","","","","","","","1.06"]
["Parametrar vid fullast och omgivningstemp. 32°C (punkt A)","R-404A","Te -35°C","Märkt kylkapacitet (PA)","kW","","","","","","","","1.42"]
["","","","Märkt ineffekt (DA)","kW","","","","","","","","1.46"]
["","","","Märkt COP (COPA)","","","","","","","","","0.97"]
["Parametrar vid fullast och omgivningstemp. 25°C","R-404A","Te -35°C","Deklarerad COP (COP2)","","","","","","","","","1.16"]
["Parameters at full load and ambient temp. 43°C","R-404A","Te -35°C","Deklarerad COP (COP3)","","","","","","","","","0.60"]