{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRMEQ-BY1"]
[]
[]
[]
[]
["","","","","","LRMEQ3BY1","LRMEQ4BY1"]
["Standardtillbehör","Installationsanvisning","","","","Installationsanvisning","Installationsanvisning"]
["","Allmänna säkerhetsföreskrifter","","","","Allmänna säkerhetsföreskrifter","Allmänna säkerhetsföreskrifter"]
["","Köldmediumsetikett för F-gasreglering","","","","Köldmediumsetikett för F-gasreglering","Köldmediumsetikett för F-gasreglering"]
["","Extra rördragningssats","","","","Extra rördragningssats","Extra rördragningssats"]
["","Avtagbar F-gas-etikett","","","","Avtagbar F-gas-etikett","Avtagbar F-gas-etikett"]
["","ecodesign produktblad","","","","ecodesign produktblad","ecodesign produktblad"]
["Kylkapacitet","Medeltemperatur","","kW","kW","5.90 (1)","8.40 (1)"]
["Vikt","Enhet","","","kg","126","126"]
["Köldmedium","Charge","","","TCO2Eq","9.39","9.39"]
["","GWP","","","","2,087.5","2,087.5"]
["","Mängd","","","kg","4.50","4.50"]
["","Typ","","","","R-410A","R-410A"]
["Fläktmotor","Utgång","","","W","70","70"]
["","Drivning","","","","Direktdriven","Direktdriven"]
["Värmeväxlare","Typ","","","","Spole med korsande flänsar","Spole med korsande flänsar"]
["Ineffekt","Medeltemperatur","","Nom.","kW","2.53 (1)","3.65 (1)"]
["COP","Medium temperature","","Nom.","","2.33 (1)","2.30 (1)"]
["Mått","Enhet","","Bredd","mm","900","900"]
["","","","Djup","mm","320","320"]
["","","","Höjd","mm","1,345","1,345"]
["Hölje","Färg","","","","Daikin vit","Daikin vit"]
["Fläkt","Typ","","","","Propeller","Propeller"]
["","Luftflödeshastighet","Kyla","Nom.","m³/min","106","106"]
["","Antal","","","","2","2"]
["Power supply","Fas","","","","3N~","3N~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","380-415","380-415"]
["Anm:","","","","","(1) - Kyla: evaporatortemp. -10℃; utomhustemp. 32 °C; insug SH10 °C","(1) - Kyla: evaporatortemp. -10℃; utomhustemp. 32 °C; insug SH10 °C"]
["","","","","","(2) - Ljudtrycksdata: uppmätt 1 m framför enheten, på 1,5 m höjd","(2) - Ljudtrycksdata: uppmätt 1 m framför enheten, på 1,5 m höjd"]
["","","","","","(3) - Innehåller fluorerande växthusgas","(3) - Innehåller fluorerande växthusgas"]