{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Standardtillbehör","Installationsanvisning","","","","1"]
["","Bruksanvisning","","","","1"]
["","Anslutningsrör","","","","1"]
["","Köldmediumsetikett för F-gasreglering","","","","1"]
["","Etikett för köldmediemängd","","","","1"]
["","Flerspråkiga etiketter om fluorerande växthusgas","","","","1"]
["Vikt","Enhet","","","kg","370"]
["Köldmedium","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Charge","","","kg","11.5"]
["","Typ","","","","R-410A"]
["Fläktmotor","Utgång","","","W","750"]
["","Drivning","","","","Direktdriven"]
["Värmeväxlare","Typ","","","","Spole med korsande flänsar"]
["Mått","Enhet","","Bredd","mm","1,240"]
["","","","Djup","mm","765"]
["","","","Höjd","mm","1,680"]
["Hölje","Färg","","","","Elfenbensvit_"]
["Fläkt","Typ","","","","Propellerfläkt"]
["","Luftflödeshastighet","Kyla","Nom.","m³/min","230"]
["","Antal","","","","2"]
["Power supply","Fas","","","","3~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","380-415"]
["Anm:","","","","","(1) - Kylprioritetsläge: inomhustemperatur. 27 °CTT, 19 °CVT; utomhustemp. 32 °CTT; rörledningslängd: 7,5m; nivåskillnad: 0m"]
["","","","","","(2) - Kylprioritetsläge: evaporatortemp. -10 ℃; utomhustemp. 32 °CTT; Insug SH: 10 ℃"]
["","","","","","(3) - Värmeåtervinning 100 % läge: inomhustemperatur. 20 °CTT; utomhustemp. 7 °CTT, 6 °CVT; kylbelastning 18 kW; rörledningslängd: 7,5m; nivåskillnad: 0m"]
["","","","","","(4) - Mättad temperatur motsvarande insugstryck (kylsidan): -10 °C (under kylda förhållanden); anslutningskapacitet för inomhus luftkonditionering: 10 HK, när värmeåtervinningen är 100 %"]
["","","","","","(5) - Kompressor 1"]
["","","","","","(6) - Kompressor 2"]
["","","","","","(7) - Kompressor 3"]
["","","","","","(8) - Enhetens fabriksmängd"]
["","","","","","(9) - Installera oljefällan 5 m från utomhusenheten"]
["","","","","","(10) - För mer information se driftsområdesritning"]
["","","","","","(11) - För mer detaljer angående standardtillbehör, se installationsmanualen/bruksanvisningen"]
["","","","","","(12) - Innehåller fluorerande växthusgas"]