{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Typ","","","","","Luftrenare"]
["Tillämpning","","","","","Golvmonterad typ"]
["Hölje","Färg","","","","Vit"]
["Mått","Enhet","","Höjd","mm","500"]
["","","","Bredd","mm","270"]
["","","","Djup","mm","270"]
["Vikt","Enhet","","","kg","6.8"]
["Tillämplig rumsstorlek","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Luftrening","Ineffekt","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","L","kW","0.010"]
["","","","Tyst","kW","0.008"]
["Ljudtrycksnivå","Luftrening","","Turbo","dBA","53"]
["","","","Medium","dBA","39"]
["","","","Låg","dBA","29"]
["","","","Tyst","dBA","19"]
["Fläkt","Luftflödeshastighet","Luftrening","Turbo","m³/h","330"]
["","","","Medium","m³/h","192"]
["","","","Låg","m³/h","120"]
["","","","Tyst","m³/h","66"]
["Dammuppsamlingsmetod","","","","","Elektrostatiskt HEPA-filter"]
["Deodorizing method","","","","","Flash streamer + luktavlägsnande katalysator"]
["Säkerhetskomponenter","Punkt","","01","","Safety switch (Operation stops when the Streamer unit cover is open)"]
["Standardtillbehör","Fjärrkontroll","","","","1"]
["","Hållare för fjärrkontroll","","","","1"]
["","Elektrostatiskt HEPA-filter","","","","1"]
["","Luktreducerande filter","","","","1"]
["","Bruksanvisning","","","","1"]
["Nätsladd","m","","","","1.8"]
["Power supply","Fas","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Spänning","","","V","220-240/220-230"]
["Belastningsström","Luftrening","","Turbo","A","0.32"]
["","","","Medium","A","0.14"]
["","","","Låg","A","0.10"]
["","","","Tyst","A","0.08"]
["Anm:","","","","","(1) - Den tillämpliga rumsarean är lämplig för att använda enheten med maximal fläkthastighet (HH). Tillämplig rumsarea indikerar den yta på vilken en viss mängd dammpartiklar kan avlägsnas på 30 minuter. (JEM 1467)"]
["","","","","","(2) - Omvandlas till NRCC-standarder från testvärden i enlighet med JEM1467."]
["","","","","","(3) - Omvandlas till CADR-standarder från testvärden i enlighet med JEM1467."]
["","","","","","(4) - Ljudnivåerna under drift är genomsnittet av de värden som uppmäts 1 m från framsidan, vänstersidan, högersidan och toppen av enheten. (Detta motsvarar värdet i en ekofri kammare)"]
["","","","","","(5) - Elektrostatiskt HEPA-filter är monterad i enheten."]
["","","","","","(6) - Andra funktioner: Aktiv formningsfunktion. Automatisk omstartsfunktion."]