{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Typ","","","","","Befuktande luftrenare"]
["Tillämpning","","","","","Golvmonterad typ"]
["Hölje","Färg","","","","Vit"]
["Mått","Enhet","","Höjd","mm","700"]
["","","","Bredd","mm","270"]
["","","","Djup","mm","270"]
["Vikt","Enhet","","","kg","9.5"]
["Tillämplig rumsstorlek","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Luftrening","Ineffekt","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Tyst","kW","0.007"]
["Befuktning","Ineffekt","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Tyst","kW","0.011"]
["","Kapacitet på vattentank","","","l","2.7"]
["Ljudtrycksnivå","Luftrening","","Turbo","dBA","53.0"]
["","","","Medium","dBA","39.0"]
["","","","Låg","dBA","29.0"]
["","","","Tyst","dBA","19.0"]
["","Befuktning","","Turbo","dBA","53.0"]
["","","","Medium","dBA","39.0"]
["","","","Låg","dBA","33.0"]
["","","","Tyst","dBA","25.0"]
["Fläkt","Luftflödeshastighet","Luftrening","Turbo","m³/h","330"]
["","","","Medium","m³/h","192"]
["","","","Låg","m³/h","120"]
["","","","Tyst","m³/h","54"]
["","","Befuktning","Turbo","m³/h","330"]
["","","","Medium","m³/h","192"]
["","","","Låg","m³/h","144"]
["","","","Tyst","m³/h","102"]
["Dammuppsamlingsmetod","","","","","Elektrostatiskt HEPA-filter"]
["Luktreduceringsmetod","","","","","Flash streamer + luktavlägsnande katalysator"]
["Standardtillbehör","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Nätsladd","Nätsladd","","","","1.8"]
["Strömförsörjning","Fas","","","","1~"]
["","Strömförsörjning-=-Frequency","","Frequency","","50/60"]
["","Strömförsörjning-=-Spänning","","Spänning","","220-240/220-230"]
["Belastningsström","Luftrening","Belastningsström-=-Luftrening-=-Turbo","Turbo","","0.50"]
["","","Belastningsström-=-Luftrening-=-Medium","Medium","","0.19"]
["","","Belastningsström-=-Luftrening-=-Låg","Låg","","0.12"]
["","","Belastningsström-=-Luftrening-=-Tyst","Tyst","","0.09"]
["","Befuktning","Belastningsström-=-Befuktning-=-Turbo","Turbo","","0.50"]
["","","Belastningsström-=-Befuktning-=-Medium","Medium","","0.20"]
["","","Belastningsström-=-Befuktning-=-Låg","Låg","","0.15"]
["","","Belastningsström-=-Befuktning-=-Tyst","Tyst","","0.13"]
["Anm:","","","","","(1) - Den tillämpliga rumsarean är lämplig för att använda enheten med maximal fläkthastighet (HH). Tillämplig rumsarea indikerar den yta på vilken en viss mängd dammpartiklar kan avlägsnas på 30 minuter. (JEM 1467)"]
["","","","","","(2) - Omvandlas till NRCC-standarder från testvärden i enlighet med JEM1467."]