{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Typ","","","","","Befuktande luftrenare"]
["Tillämpning","","","","","Golvmonterad typ"]
["Hölje","Färg","","","","Vit (N9. 0)"]
["Mått","Enhet","","Höjd","mm","600 (5)"]
["","","","Bredd","mm","395"]
["","","","Djup","mm","287"]
["Vikt","Enhet","","","kg","12.5"]
["Tillämplig rumsstorlek","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Luftrening","Ineffekt","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Tyst","kW","0.008"]
["Befuktning","Ineffekt","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Tyst","kW","0.011"]
["","Kapacitet på vattentank","","","l","3.6"]
["Ljudtrycksnivå","Luftrening","","Turbo","dBA","54"]
["","","","Medium","dBA","37"]
["","","","Låg","dBA","27"]
["","","","Tyst","dBA","18"]
["","Befuktning","","Turbo","dBA","54"]
["","","","Medium","dBA","37"]
["","","","Låg","dBA","27"]
["","","","Tyst","dBA","23"]
["Fläkt","Luftflödeshastighet","Luftrening","Turbo","m³/h","420"]
["","","","Medium","m³/h","210"]
["","","","Låg","m³/h","132"]
["","","","Tyst","m³/h","60"]
["","","Befuktning","Turbo","m³/h","420"]
["","","","Medium","m³/h","210"]
["","","","Låg","m³/h","132"]
["","","","Tyst","m³/h","102"]
["Dammuppsamlingsmetod","","","","","Elektrostatiskt HEPA-filter"]
["Luktreduceringsmetod","","","","","Flash streamer + luktavlägsnande katalysator"]
["Standardtillbehör","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Nätsladd","m","","","","2"]
["Strömförsörjning","Fas","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Spänning","","","V","220-240/220-230"]
["Anm:","","","","","(1) - Täckningsarean är lämplig för att använda enheten med maximal fläkthastighet (HH). Täckningsarean indikerar den yta på vilken en viss mängd dammpartiklar kan avlägsnas på 30 minuter."]
["","","","","","(2) - Omvandlas till NRCC-standarder från testvärden i enlighet med JEM1467."]
["","","","","","(3) - Ljudnivåerna under drift är genomsnittet av de värden som uppmäts 1 m från framsidan, vänstersidan, högersidan och toppen av enheten. (Detta motsvarar värdet i en ekofri kammare)"]