{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":20,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RX-K"]
[]
[]
[]
[]
["","","","","","RX20K2V1B","RX20K5V1B","RX20K5V1B9","RX25K2V1B","RX25K5V1B","RX25K5V1B9","RX35K2V1B","RX35K5V1B","RX35K5V1B9","RX50KV1B","RX50K2V1B","RX60KV1B","RX60K2V1B","RX71KV1B","RX71K2V1B"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","","","","","","","","","","51.3"]
["","","Värme","Superlåg","m³/min","","","","","","","","","","51.3"]
["","","","Superlåg","cfm","","","","","","","","","","1812"]
["","","Värme","Superlåg","cfm","","","","","","","","","","1812"]
["Mått","Enhet","","Höjd","mm","550","550","550","550","550","550","550","550","550","735","734","735","734","735","734"]
["","","","Bredd","mm","658","658","658","658","658","658","658","658","658","870","870","870","870","870","870"]
["","","","Djup","mm","275","275","275","275","275","275","275","275","275","320","373","320","373","320","373"]
["Vikt","Enhet","","","kg","28","28","28","28","28","28","28","28","28","44","46.0","49","49.0","49","49.0"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10","","-10"]
["","","","Max.","°CTT","46","46","46","46","46","46","46","46","46","46","","46"]
["","Värme","Omgivning","Min.","°CVT","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","","-15"]
["","","","Max.","°CVT","18","18","18","18","18","18","18","18","18","18","","18"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","46","46","46","46","46","46","48","48","48","47","","49","","52"]
["","","","Nom.","dBA","","","","","","","","","","","47","","49","","52"]
["","Värme","","Hög","dBA","47","47","47","47","47","47","48","48","48","48","","49","","52"]
["","","","Nom.","dBA","","","","","","","","","","","48","","49","","52"]
["Köldmedium","Typ","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Mängd","","","kg","0.74","0.74","0.74","0.74","0.74","0.74","1.0","1.0","1.0","1.13","1.13","1.45","1.45","1.45","1.45"]
["","Mängd","","","tCO2Eq","1.5","1.5","1.5","1.5","1.5","1.5","2.1","2.1","2.1","2.4","2.36","3.0","3.03","3.0","3.03"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","15","15","15","15","15","15","15","15","15","30","30.0","30","30.0","30","30.0"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","12","12","12","12","12","12","12","12","12","20","20.0","20","20.0","20","20.0"]
["Standardtillbehör","Installation manual","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["Strömförsörjning","Fas","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Anm:","","","","","(1) - Driftsområde i kombination med FTX-J3: min. 10°CTT ~ max. 46°CTT","(1) - Driftsområde i kombination med FTX-J3: min. 10°CTT ~ max. 46°CTT","(1) - Driftsområde i kombination med FTX-J3: min. 10°CTT ~ max. 46°CTT","(1) - Driftsområde i kombination med FTX-J3: min. 10°CTT ~ max. 46°CTT","(1) - Driftsområde i kombination med FTX-J3: min. 10°CTT ~ max. 46°CTT","(1) - Driftsområde i kombination med FTX-J3: min. 10°CTT ~ max. 46°CTT","(1) - Driftsområde i kombination med FTX-J3: min. 10°CTT ~ max. 46°CTT","(1) - Driftsområde i kombination med FTX-J3: min. 10°CTT ~ max. 46°CTT","(1) - Driftsområde i kombination med FTX-J3: min. 10°CTT ~ max. 46°CTT"]
["Standardtillbehör","Drain cap","","","","","","","","","","","","","9","9","9","9","9","9"]