{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":9,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B2V1B","RXA42B5V1B","RXA50B2V1B","RXA50B5V1B"]
["Mått","Enhet","","Höjd","mm","734","","734","734"]
["","","","Bredd","mm","870","","870","954"]
["","","","Djup","mm","373","","373","401"]
["Vikt","Enhet","","","kg","50","","50","49"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10","","-10","-10"]
["","","","Max.","°CTT","46","","46","46"]
["","Värme","Omgivning","Min.","°CVT","-15","","-15","-15"]
["","","","Max.","°CVT","18","","18","18"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","48.0","","48.0","48"]
["","Värme","","Nom.","dBA","48.0","","48.0","48"]
["Köldmedium","Typ","","","","R-32","","R-32","R-32"]
["","Mängd","","","kg","1.10","","1.10","1.1"]
["","Mängd","","","tCO2Eq","0.75","","0.75","0.75"]
["","GWP","","","","675","","675","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","30","","30","30"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","20","","20","20"]
["Standardtillbehör","Installationsanvisning","","","","1","","1","1"]
["","Etikett för köldmediemängd","","","","1","","1","1"]
["","Flerspråkiga etiketter om fluorerande växthusgas","","","","1","","1","1"]
["","Kondensvattenplugg","","","","1","","1","1"]
["Intervall för energieffektivitet","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Strömförsörjning","Fas","","","","1~","","1~","1~"]
["","Frequency","","","Hz","50","","50","50"]
["","Spänning","","","V","220-240","","220-240","220-240"]
["Anm:","","","","","(1) - Se separat ritning för driftsområde","","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde"]
["","","","","","(2) - Se separata ritningar för elektriska data","","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data"]
["","","","","","(3) - Innehåller fluorerande växthusgas","","(3) - Innehåller fluorerande växthusgas","(3) - Innehåller fluorerande växthusgas"]