{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":16,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-M"]
[]
[]
[]
[]
["","","","","","RXJ20M2V1B","RXJ20M3V1B","RXJ20M5V1B","RXJ25M2V1B","RXJ25M3V1B","RXJ25M5V1B","RXJ35M2V1B","RXJ35M3V1B","RXJ35M5V1B","RXJ50MV1B","RXJ50M2V1B"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","29.3","","","29.3","","","29.3","","","38.5"]
["","","Värme","Superlåg","m³/min","25.6","","","25.6","","","25.6","","","34.3"]
["","","","Superlåg","cfm","1035","","","1035","","","1035","","","1359"]
["","","Värme","Superlåg","cfm","904","","","904","","","904","","","1211"]
["Mått","Enhet","","Höjd","mm","550","550","550","550","550","550","550","550","550","735","735"]
["","","","Bredd","mm","765","765","765","765","765","765","765","765","765","825","825"]
["","","","Djup","mm","285","285","285","285","285","285","285","285","285","300","300"]
["Vikt","Enhet","","","kg","34","32","32","34","32","32","34","32","32","44","44"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","760","","","760","","","760","","","620"]
["","","Värme","Superlåg","varv/min","740","","","740","","","740","","","620"]
["Kompressor","Type","","","","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CTT","46","46","46","46","46","46","46","46","46","46","46"]
["","Värme","Omgivning","Min.","°CVT","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CVT","18","18","18","18","18","18","18","18","18","18","20"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","46","","","46","","","48","","","48","48"]
["","","","Nom.","dBA","","46","46","","46","46","","49","49"]
["","","","Låg","dBA","","","","","","","","","","","45"]
["","Värme","","Hög","dBA","47","","","47","","","48","","","48","48"]
["","","","Nom.","dBA","","47","47","","47","47","","49","49"]
["","","","Låg","dBA","","","","","","","","","","","45"]
["Köldmedium","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Mängd","","","kg","0.72","0.76","0.76","0.72","0.76","0.76","0.72","0.76","0.76","1.30","1.3"]
["","Mängd","","","tCO2Eq","0.5","0.52","0.52","0.5","0.52","0.52","0.5","0.52","0.52","0.9","0.88"]
["","GWP","","","","675","675.0","675.0","675","675.0","675.0","675","675.0","675.0","675","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20","20","20","20","20","20","20","20","20","30","30"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","15","15.0","15.0","15","15.0","15.0","15","15.0","15.0","20"]
["Standardtillbehör","Installation manual","","","","1","1","","1","1","","1","1","","1"]
["","Drain plug","","","","1","1","","1","1","","1","1","","1"]
["Strömförsörjning","Fas","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Anm:","","","","","(1) - 220V","","","(1) - 220V","","","(1) - 220V","","","(1) - 220V"]
["","","","","","(2) - 230V","","","(2) - 230V","","","(2) - 230V","","","(2) - 230V"]
["","","","","","(3) - 240V","","","(3) - 240V","","","(3) - 240V","","","(3) - 240V"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Standardtillbehör","Refrigerant charge label","","","","","1","","","1","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","","","1","","","1"]
["","General safety precautions","","","","","1","","","1","","","1"]