{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","30.6","30.6"]
["","","Värme","Superlåg","m³/min","27.2","27.2"]
["","","","Superlåg","cfm","1080","1080"]
["","","Värme","Superlåg","cfm","960","960"]
["Mått","Enhet","","Höjd","mm","550","550"]
["","","","Bredd","mm","858","858"]
["","","","Djup","mm","330","330"]
["Vikt","Enhet","","","kg","40","40"]
["Kompressor","Type","","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10","-10"]
["","","","Max.","°CTT","46","46"]
["","Värme","Omgivning","Min.","°CVT","-25","-25"]
["","","","Max.","°CVT","18","18"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","48","48"]
["","","","Låg","dBA","44","44"]
["","Värme","","Hög","dBA","49","49"]
["","","","Låg","dBA","45","45"]
["Köldmedium","Typ","","","","R-410A","R-410A"]
["","Mängd","","","kg","1","1"]
["","Mängd","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20","20"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - IU","Max.","m","15","15"]
["Standardtillbehör","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Strömförsörjning","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","220-240","220-240"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor"]