{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":12,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A"]
[]
[]
[]
[]
["","","","","","RXM20A5V1B","RXM25A5V1B","RXM35A5V1B","RXM42A5V1B","RXM50A5V1B","RXM60A5V1B","RXM71A5V1B"]
["Mått","Enhet","","Höjd","mm","610","610","610","610","734","734","734"]
["","","","Bredd","mm","923","923","923","923","954","954","954"]
["","","","Djup","mm","367","367","367","367","401","401","401"]
["Vikt","Enhet","","","kg","36","36","36","40","49","49","55"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","600","600","600","600","500"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CDB","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","50","50","50","50","50 (1)","50","46"]
["","Värme","Omgivning","Min.","°CVT","-21","-21","-21","-21","-21 (1)","-21","-15"]
["","","","Max.","°CVT","18","18","18","18","18","18","18"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","46","46","47","48","48","48","47"]
["","Värme","","Nom.","dBA","47","47","49","49","49","49","48"]
["Köldmedium","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Mängd","","","kg","0.95","0.95","0.95","0.95","1.10","1.15","1.15"]
["","Mängd","","","tCO2Eq","0.65","0.65","0.65","0.65","0.75","0.78","0.78"]
["","GWP","","","","675","675","675","675","675","675","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20","20","20","30","30","30","30"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","15","15","15","20","20","20","20"]
["Strömförsörjning","Fas","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardtillbehör","Installation manual","","","","1","1","1","1","1","1","1"]
["","Drain joint","","","","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1","1"]
["","Drain cap","","","","3","3","3","3","1","3","3"]
["Anm:","","","","","","","","","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde"]
["","","","","","","","","","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data"]
["","","","","","","","","","(3) - Innehåller fluorerande växthusgas","(3) - Innehåller fluorerande växthusgas","(3) - Innehåller fluorerande växthusgas"]
["Standardtillbehör","Drain plug","","","","","","","","","1","1"]