{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":15,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-R"]
[]
[]
[]
[]
["","","","","","RXM20R5V1B","RXM25R5V1B","RXM35R5V1B","RXM42R2V1B","RXM42R5V1B","RXM50R2V1B","RXM50R5V1B","RXM60R2V1B","RXM60R5V1B","RXM71R2V1B"]
["Mått","Enhet","","Höjd","mm","552","552","552","734","734","734","734","734","734","734"]
["","","","Bredd","mm","840","840","840","954","954","954","954","954","954","954"]
["","","","Djup","mm","350","350","350","401","401","401","401","401","401","401"]
["Vikt","Enhet","","","kg","32","32","32","49.0","49.0","49.0","49.0","49.0","49.0","55"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CTT","50 (4), 46 (5)","50 (4), 46 (5)","50 (4), 46 (5)","50, 46","50, 46","50, 46","50, 46","50, 46","50, 46","46"]
["","Värme","Omgivning","Min.","°CWB","-15","-15","-15","-15","-21","-15","-21","-15","-21","-15"]
["","","","Max.","°CWB","18","18","18","18","18","18","18","18","18","18"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","46","46","49","48.0","48.0","48.0","48.0","48.0","48.0","47.0"]
["","Värme","","Nom.","dBA","47","47","49","48.0","48.0","49.0","49.0","49.0","49.0","48.0"]
["Köldmedium","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Mängd","","","kg","0.76","0.76","0.76","1.10","1.10","1.15","1.15","1.15","1.15","1.15"]
["","Mängd","","","tCO2Eq","0.52","0.52","0.52","0.750","0.750","0.780","0.780","0.780","0.780","0.780"]
["","GWP","","","","675","675","675","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20","20","20","30","30","30","30","30","30","30"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","15","15","15","20.0","20.0","20.0","20.0","20.0","20.0","20.0"]
["Standardtillbehör","Installation manual","","","","1","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1","1","1","1"]
["Strömförsörjning","Fas","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Anm:","","","","","(1) - Endast möjlig i kombination med CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Endast möjlig i kombination med CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Endast möjlig i kombination med CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B"]
["","","","","","(2) - Endast möjlig i kombination med CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9,FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB·","(2) - Endast möjlig i kombination med CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9,FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB·","(2) - Endast möjlig i kombination med CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9,FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB·"]
["Standardtillbehör","Drain cap","","","","","","","3","3","3","3","3","3","3"]