{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":6,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N8"]
[]
[]
[]
[]
["","","","","","RXP50N5V1B8"]
["Mått","Enhet","","Höjd","mm","610"]
["","","","Bredd","mm","923"]
["","","","Djup","mm","367"]
["Vikt","Enhet","","","kg","40"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","600"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10"]
["","","","Max.","°CTT","48"]
["","Värme","Omgivning","Min.","°CVT","-15"]
["","","","Max.","°CVT","18"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","48"]
["","Värme","","Nom.","dBA","49"]
["Köldmedium","Typ","","","","R-32"]
["","Mängd","","","kg","0.95"]
["","Mängd","","","tCO2Eq","0.65"]
["","GWP","","","","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","30"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","20"]
["Standardtillbehör","RXP50N5V1B8","","","","3"]
["","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["Strömförsörjning","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","(1) - Se separat ritning för driftsområde"]
["","","","","","(2) - Se separata ritningar för elektriska data"]
["","","","","","(3) - Innehåller fluorerande växthusgas"]