{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":11,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N9"]
[]
[]
[]
[]
["","","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9","RXP50N5V1B9","RXP60N5V1B9","RXP71N5V1B9"]
["Mått","Enhet","","Höjd","mm","556","556","556","734","734","734"]
["","","","Bredd","mm","740","740","740","954","954","954"]
["","","","Djup","mm","343","343","343","401","401","401"]
["Vikt","Enhet","","","kg","24","24","26","46","50","50"]
["Kompressor","Type","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CTT","48","48","48","48","48","48"]
["","Värme","Omgivning","Min.","°CVT","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CVT","18","18","18","18","18","18"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","46","46","48"]
["","","","Nom.","dBA","","","","47","49","52"]
["","Värme","","Hög","dBA","47","47","48"]
["","","","Nom.","dBA","","","","49","49","52"]
["Köldmedium","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Mängd","","","kg","0.55","0.55","0.70","0.9","1.15","1.15"]
["","Mängd","","","tCO2Eq","0.37","0.37","0.48","0.61","0.78","0.78"]
["","GWP","","","","675.0","675.0","675.0","675","675","675"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20","20","20","30","30","30"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","12","12","12","20","20","20"]
["Standardtillbehör","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Strömförsörjning","Fas","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardtillbehör","Drain cap","","","","","","","3","3","3"]
["Anm:","","","","","","","","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde"]
["","","","","","","","","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data"]
["","","","","","","","","(3) - Innehåller fluorerande växthusgas","(3) - Innehåller fluorerande växthusgas","(3) - Innehåller fluorerande växthusgas"]