{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","49","","","52"]
["","","","Låg","dBA","46","","","49"]
["","Kyla","","Låg","dBA","46","","","49"]
["","","","Hög","dBA","49","","","52"]
["Standardtillbehör","Kondensvattenuttag","","","","1","","","1"]
["","Installationsanvisning","","","","1","","","1"]
["Köldmedium","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Mängd","","","kg","1.5","","","2.3"]
["","Typ","","","","R-410A","","","R-410A"]
["Röranslutningar","Nivåskillnad","IU - OU","Max.","m","20","","","20"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","","","0,02 (för rördragning över 10m)"]
["Ljudeffektsnivå","Kyla","","","dBA","","","","65"]
["Kompressor","Type","","","","Hermetiskt tillsluten swing-kompressor","","","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Bredd","mm","825","","","900"]
["","","","Djup","mm","300","","","320"]
["","","","Höjd","mm","735","","","770"]
["Vikt","Enhet","","","kg","48","","","71"]
["Power supply","Phase","","","","1~","","","1~"]
["","Frequency","","","Hz","50","","","50"]
["","Spänning","","","V","220-240","","","220-240"]
["Anm:","","","","","(1) - SL: Den tysta fläktnivån av luftflödeshastighetsinställningen","(1) - 220V","","(1) - SL: Den tysta fläktnivån av luftflödeshastighetsinställningen","(1) - 220V"]
["","","","","","(2) - Innehåller fluorerande växthusgas","(2) - 230V","","(2) - Innehåller fluorerande växthusgas","(2) - 230V"]
["Mått","Enhet","","Höjd","mm","","735","735","","770","770"]
["","","","Bredd","mm","","825","825","","900","900"]
["","","","Djup","mm","","300","300","","320","320"]
["Vikt","Enhet","","","kg","","48","48","","71","71"]
["Kompressor","Type","","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","","-10","-10","","-10","-10"]
["","","","Max.","°CTT","","46","46","","46","46"]
["","Värme","Omgivning","Min.","°CVT","","-15","-15","","-15","-15"]
["","","","Max.","°CVT","","18","20","","18","20"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","49","49","","52","52"]
["","","","Låg","dBA","","46","46","","49","49"]
["","Värme","","Hög","dBA","","49","49","","52","52"]
["","","","Låg","dBA","","46","46","","49","49"]
["Köldmedium","Typ","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Mängd","","","kg","","1.5","1.5","","2.3","2.3"]
["","Mängd","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","","30","30","","30","30"]
["","Extra köldmediemängd","","","kg/m","","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","","20","20","","20","20"]
["Standardtillbehör","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Strömförsörjning","Fas","","","","","1~","1~","","1~","1~"]
["","Frequency","","","Hz","","50","50","","50","50"]
["","Spänning","","","V","","220-240","220-240","","220-240","220-240"]
["Anm:","","","","","","(3) - 240V","","","(3) - 240V"]
["Standardtillbehör","Drain socket","","","","","","1","","","1"]