{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","46.0"]
["","","Värme","Superlåg","m³/min","46.0"]
["","","","Superlåg","cfm","1624"]
["","","Värme","Superlåg","cfm","1624"]
["Mått","Enhet","","Höjd","mm","770"]
["","","","Bredd","mm","900"]
["","","","Djup","mm","320"]
["Vikt","Enhet","","","kg","71"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min (2)","730"]
["","","Värme","Superlåg","varv/min (2)","730"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-10"]
["","","","Max.","°CTT","46"]
["","Värme","Omgivning","Min.","°CVT","-15"]
["","","","Max.","°CVT","18"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","52"]
["","Värme","","Hög","dBA","52"]
["Köldmedium","Typ","","","","R-410A"]
["","Mängd","","","kg","2.3"]
["","Mängd","","","tCO2Eq","4.8"]
["","GWP","","","","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","30"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","20"]
["Standardtillbehör","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Strömförsörjning","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]