{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","47","","47","","48","48","48"]
["","Kyla","","Hög","dBA","46","","46","","48","48","48"]
["Standardtillbehör","Anslutning (dränering)","","","","1","","1"]
["","Installationsanvisning","","","","1","","1","","1","1","1"]
["Köldmedium","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Typ","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","780","","780","","780","790","670"]
["","","Värme","Superlåg","varv/min","740","","740","","740","780","670"]
["Röranslutningar","Nivåskillnad","IU - OU","Max.","m","15","","15","","15","15","20"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","","0,02 (för rördragning över 10m)","","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","","Hermetiskt tillsluten swing-kompressor","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Bredd","mm","765","","765","","765","765","825"]
["","","","Djup","mm","285","","285","","285","285","300"]
["","","","Höjd","mm","550","","550","","550","550","735"]
["Vikt","Enhet","","","kg","34","","34","","34","39","47"]
["Fläkt","Luftflödeshastighet","Värme","Superlåg","cfm","","","","","904","960","1,522"]
["","","Kyla","Superlåg","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Fas","","","","1~","","1~","","1~","1~","1~"]
["","Frequency","","","Hz","50","","50","","50","50","50"]
["","Spänning","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Anm:","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL: Den tysta fläktnivån av luftflödeshastighetsinställningen","","(4) - SL: Den tysta fläktnivån av luftflödeshastighetsinställningen","","(4) - Innehåller fluorerande växthusgas","(4) - Innehåller fluorerande växthusgas","(4) - Innehåller fluorerande växthusgas"]
["","","","","","(5) - Innehåller fluorerande växthusgas","","(5) - Innehåller fluorerande växthusgas"]
["Mått","Enhet","","Höjd","mm","","550","","550"]
["","","","Bredd","mm","","765","","765"]
["","","","Djup","mm","","285","","285"]
["Vikt","Enhet","","","kg","","34","","34"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","","780","","780"]
["","","Värme","Superlåg","varv/min","","740","","740"]
["Kompressor","Typ","","","","","Hermetiskt tillsluten swing-kompressor","","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CDB","","-10","","-10"]
["","","","Max.","°CDB","","46","","46"]
["","Värme","Omgivning","Min.","°CVT","","-15","","-15"]
["","","","Max.","°CVT","","18","","18"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","46","","46"]
["","Värme","","Hög","dBA","","47","","47"]
["Köldmedium","Typ","","","","","R-410A","","R-410A"]
["","Mängd","","","kg","","1.0","","1.0"]
["","Mängd","","","tCO2Eq","","2.1","","2.1"]
["","GWP","","","","","2087.5","","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","","20","","20"]
["","Extra köldmediemängd","","","kg/m","","0,02 (för rördragning över 10m)","","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","","15","","15"]
["Standardtillbehör","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Strömförsörjning","Fas","","","","","1~","","1~"]
["","Frequency","","","Hz","","50","","50"]
["","Spänning","","","V","","220-240","","220-240"]
["Standardtillbehör","Kondensvattenplugg","","","","","","","","1","1","1"]