{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":11,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","47","47","48","48"]
["","Kyla","","Hög","dBA","46","46","48","48"]
["Standardtillbehör","Kondensvattenplugg","","","","1","1","1","1"]
["","Installationsanvisning","","","","1","1","1","1"]
["","Etikett för köldmediemängd","","","","1","1","1"]
["","Flerspråkiga etiketter om fluorerande växthusgas","","","","1","1","Flerspråkiga etiketter om fluorerande växthusgas"]
["Köldmedium","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Mängd","","","kg","1.0","1.0","1.20","1.3"]
["","Typ","","","","R-410A","R-410A","R-410A","R-410A"]
["Fläktmotor","Varvtal","Kyla","Superlåg","varv/min","780","780","780","790"]
["","","Värme","Superlåg","varv/min","740","740","740","780"]
["Driftsområde","Kyla","Omgivning","Max.","°CTT","46","46","46","46"]
["","","","Min.","°CTT","-10","-10","-10","-10"]
["","Heating","Omgivning","Max.","°CVT","18","18","18","18"]
["","","","Min.","°CVT","-15","-15","-15","-15"]
["Röranslutningar","Nivåskillnad","IU - OU","Max.","m","","","15"]
["","Extra köldmediemängd","","","kg/m","","","0,020 (för rördragning över 10 m)"]
["Mått","Enhets-","","Bredd","mm","765","765","765","765"]
["","","","Djup","mm","285","285","285","285"]
["","","","Höjd","mm","550","550","550","550"]
["Kompressor","Type","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Vikt","Enhet","","","kg","34","34","34","39"]
["Fläkt","Luftflödeshastighet","Värme","Superlåg","cfm","904","904","904","960"]
["","","","Superlåg","m³/min","25.6","25.6","25.6","27.2"]
["","","Kyla","Superlåg","m³/min","30.1","30.1","30.1","30.6"]
["","","","Superlåg","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240","220-240"]
["Anm:","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Innehåller fluorerande växthusgas","(4) - Innehåller fluorerande växthusgas","(4) - Innehåller fluorerande växthusgas","(4) - Innehåller fluorerande växthusgas"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","","","","","48.9","45.0"]
["","","Värme","Superlåg","m³/min","","","","","43.1","46.3"]
["","","","Superlåg","cfm","","","","","1727","1589"]
["","","Värme","Superlåg","cfm","","","","","1522","1635"]
["Mått","Enhet","","Höjd","mm","","","","","735","735"]
["","","","Bredd","mm","","","","","825","825"]
["","","","Djup","mm","","","","","300","300"]
["Vikt","Enhet","","","kg","","","","","47","48"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","","","","","670"]
["","","Värme","Superlåg","varv/min","","","","","670"]
["Kompressor","Typ","","","","","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","","","","","-10","-10"]
["","","","Max.","°CTT","","","","","46","46"]
["","Värme","Omgivning","Min.","°CVT","","","","","-15","-15"]
["","","","Max.","°CVT","","","","","18","18"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","","","","48","49"]
["","","","Låg","dBA","","","","","44","46"]
["","Värme","","Hög","dBA","","","","","48","49"]
["","","","Låg","dBA","","","","","45","46"]
["Köldmedium","Typ","","","","","","","","R-410A","R-410A"]
["","Mängd","","","kg","","","","","1.7","1.5"]
["","Mängd","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","","","","","30","30"]
["","Extra köldmediemängd","","","kg/m","","","","","0,020 (för rördragning över 10 m)","0,020 (för rördragning över 10 m)"]
["","Nivåskillnad","IU - OU","Max.","m","","","","","20.0","20"]
["Standardtillbehör","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Strömförsörjning","Fas","","","","","","","","1~","1~"]
["","Frequency","","","Hz","","","","","50","50"]
["","Spänning","","","V","","","","","220-230-240","220-230-240"]
["Anm:","","","","","","","","","","(1) - 230V"]