{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","","","48"]
["","Kyla","","Hög","dBA","","","48"]
["Standardtillbehör","Installationsanvisning","","","","","","1"]
["","Etikett för köldmediemängd","","","","","","1"]
["","Flerspråkiga etiketter om fluorerande växthusgas","","","","","","1"]
["","Dräneringsplugg (endast värmepumpsmodeller)","","","","","","1"]
["Köldmedium","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Mängd","","","kg","","","1.2"]
["","Typ","","","","","","R-410A"]
["Fläktmotor","Varvtal","Kyla","Superlåg","varv/min","","","780"]
["","","Värme","Superlåg","varv/min","","","740"]
["Driftsområde","Kyla","Omgivning","Max.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Heating","Omgivning","Max.","°CVT","","","18"]
["","","","Min.","°CVT","","","-15"]
["Röranslutningar","Nivåskillnad","IU - OU","Max.","m","","","15"]
["","Extra köldmediemängd","","","kg/m","","","0,02 (för rördragning över 10m)"]
["Mått","Enhet","","Bredd","mm","","","765"]
["","","","Djup","mm","","","285"]
["","","","Höjd","mm","","","550"]
["Compressor","Type","","","","","","Hermetiskt tillsluten swing-kompressor"]
["Vikt","Enhet","","","kg","","","34"]
["Fläkt","Luftflödeshastighet","Värme","Superlåg","cfm","","","904"]
["","","","Superlåg","m³/min","","","25.6"]
["","","Kyla","Superlåg","m³/min","","","30.1"]
["","","","Superlåg","cfm","","","1,063"]
["Power supply","Phase","","","","","","1~"]
["","Frequency","","","Hz","","","50"]
["","Spänning","","","V","","","220-240"]
["Anm:","","","","","","","(1) - SL: Den tysta fläktnivån av luftflödeshastighetsinställningen"]
["Fläkt","Luftflödeshastighet","Kyla","Superlåg","m³/min","30.1","30.1"]
["","","Värme","Superlåg","m³/min","25.6","25.6"]
["","","","Superlåg","cfm","1063","1063"]
["","","Värme","Superlåg","cfm","904","904"]
["Mått","Enhet","","Höjd","mm","550","550"]
["","","","Bredd","mm","765","765"]
["","","","Djup","mm","285","285"]
["Vikt","Enhet","","","kg","34","34"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","780","780"]
["","","Värme","Superlåg","varv/min","740","740"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Värme","Omgivning","Min.","°CVT","-15","-15"]
["","","","Max.","°CVT","18","18"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","46","46"]
["","Värme","","Hög","dBA","47","47"]
["Köldmedium","Typ","","","","R-410A","R-410A"]
["","Mängd","","","kg","1.0","1.0"]
["","Mängd","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Röranslutningar","Rörledningslängd","Max.","UE - IE","m","20","20"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["","Nivåskillnad","IU - OU","Max.","m","15","15"]
["Standardtillbehör","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Strömförsörjning","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","220-240","220-240"]
["Anm:","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]
["Standardtillbehör","Drain plug (only heat pump models)","","","","","1"]