{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Mått","Enhet","","Höjd","mm","870","870"]
["","","","Bredd","mm","1,100","1,100"]
["","","","Djup","mm","460","460"]
["Vikt","Enhet","","","kg","117","117"]
["Kompressor","Type","","","","Hermetiskt försluten scrollkompressor","Hermetiskt försluten scrollkompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-20","-20"]
["","","","Max.","°CTT","46","46"]
["","Värme","Omgivning","Min.","°CVT","-20","-20"]
["","","","Max.","°CVT","15","15"]
["Ljudeffektsnivå","Kyla","","","dBA","73","76"]
["","Värme","","","dBA","76 (1)","79 (1)"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","53","57"]
["","Värme","","Nom.","dBA","60","63"]
["Köldmedium","Typ","","","","R-32","R-32"]
["","Mängd","","","kg","5","5"]
["","GWP","","","","675","675"]
["Röranslutningar","Vätska","","YD","mm","9.52","9.52"]
["","Gas","","YD","mm","22.2","22.2"]
["","Rörledningslängd","Max.","UE - IE","m","100","100"]
["","","System","Ingen extra laddning","m","30","30"]
["","Extra köldmediemängd","","","kg/m","Se installationsmanual","Se installationsmanual"]
["Standardtillbehör","Installationsanvisning","","","","1","1"]
["","Allmänna säkerhetsföreskrifter","","","","1","1"]
["","Buntband","","","","2","2"]
["","Avtagbar F-gas-etikett","","","","1","1"]
["","Anslutningsrör","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","380-415","380-415"]
["Ström - 50Hz","Max amperestyrka i säkring (MFA)","","","A","20","20"]
["Anm:","","","","","(1) - Enligt ENER Lot 21","(1) - Enligt ENER Lot 21"]