{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Mått","Enhet","","Höjd","mm","734","734","734"]
["","","","Bredd","mm","870","870","870"]
["","","","Djup","mm","373","373","373"]
["Vikt","Enhet","","","kg","52","52","52"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-20","-20","-20"]
["","","","Max.","°CTT","52","52","52"]
["","Värme","Omgivning","Min.","°CVT","-21","-21","-21"]
["","","","Max.","°CVT","18","18","18"]
["Ljudeffektsnivå","Kyla","","","dBA","62","63","64"]
["","Värme","","","dBA","62","63","64"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","48","49","50"]
["","Värme","","Nom.","dBA","48","49","50"]
["Köldmedium","Typ","","","","R-32","R-32","R-32"]
["","Mängd","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Mängd","","","tCO2Eq","1.05","1.05","1.05"]
["Röranslutningar","Vätska","","YD","mm","6.35","6.35","6.35"]
["","Gas","","YD","mm","9.52","12.7","12.7"]
["","Rörledningslängd","Max.","UE - IE","m","50","50","50"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 30m)","0,02 (för rördragning över 30m)","0,02 (för rördragning över 30m)"]
["","Nivåskillnad","IU - OU","Max.","m","30","30","30"]
["Standardtillbehör","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Strömförsörjning","Fas","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240"]
["Anm:","","","","","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde","(1) - Se separat ritning för driftsområde"]
["","","","","","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data","(2) - Se separata ritningar för elektriska data"]
["","","","","","(3) - Innehåller fluorerande växthusgas","(3) - Innehåller fluorerande växthusgas","(3) - Innehåller fluorerande växthusgas"]
["Standardtillbehör","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]