{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B","RZAG140M7V1B"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","","","","52"]
["","Kyla","","Nom.","dBA","","","","51"]
["Standardtillbehör","Buntband","","","","","","","2"]
["","Installationsanvisning","","","","","","","1"]
["","Köldmediumsetikett för F-gasreglering","","","","","","","1"]
["","Allmänna säkerhetsföreskrifter","","","","","","","1"]
["","LOT10 Energiklass","","","","","","","1"]
["Köldmedium","Charge","","","TCO2Eq","","","","2.53"]
["","GWP","","","","","","","675"]
["","Charge","","","kg","","","","3.75"]
["","Typ","","","","","","","R-32"]
["Röranslutningar","Vätska","","YD","mm","","","","9.52"]
["","Rörledningslängd","Max.","UE - IE","m","","","","85"]
["","","System","Ingen extra laddning","m","","","","40"]
["","","","Motsvarande","m","","","","100"]
["","Gas","","YD","mm","","","","15.9"]
["","Nivåskillnad","IU - IU","Max.","m","","","","0.5"]
["","","IU - OU","Max.","m","","","","30.0"]
["","Extra köldmediemängd","","","kg/m","","","","Se installationsmanual"]
["Ljudeffektsnivå","Kyla","","","dBA","","","","70"]
["","Värme","","","dBA","","","","70 (1)"]
["Kompressor","Typ","","","","","","","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Bredd","mm","","","","940"]
["","","","Djup","mm","","","","320"]
["","","","Höjd","mm","","","","1,430"]
["Vikt","Enhet","","","kg","","","","92"]
["Power supply","Fas","","","","","","","1~"]
["","Frequency","","","Hz","","","","50"]
["","Spänning","","","V","","","","220-240"]
["Anm:","","","","","","","","(1) - Enligt ENER Lot 21"]
["","","","","","","","","(2) - Europeisk/internationell teknisk standard sätter gränserna för harmoniska strömmar som produceras av utrustning ansluten till det publika lågspänningssystemet med ingångsström högre än16 A och ≤75 A per fas"]
["","","","","","","","","(3) - Ssc: kortsluten spänning"]
["","","","","","","","","(4) - Europeisk/internationell teknisk standard sätter gränserna för harmoniska strömmar som produceras av utrustning ansluten till det publika lågspänningssystemet med ingångsström ≤16 A per fas"]
["Mått","Enhet","","Höjd","mm","990","1430","1430"]
["","","","Bredd","mm","940","940","940"]
["","","","Djup","mm","320","320","320"]
["Vikt","Enhet","","","kg","70","92","92"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CDB","-20","-20","-20"]
["","","","Max.","°CDB","52","52","52"]
["","Värme","Omgivning","Min.","°CVT","-20","-20","-20"]
["","","","Max.","°CVT","18.0","18.0","18.0"]
["Ljudeffektsnivå","Kyla","","","dBA","64","66","69"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","46","47","50"]
["","Värme","","Nom.","dBA","49","51","52"]
["Köldmedium","Typ","","","","R-32","R-32","R-32"]
["","Mängd","","","kg","2.95","3.75","3.75"]
["","GWP","","","","675","675","675"]
["","Mängd","","","tCO2Eq","1.99","2.53","2.53"]
["Röranslutningar","Vätska","","YD","mm","9.52","9.52","9.52"]
["","Gas","","YD","mm","15.9","15.9","15.9"]
["","Rörledningslängd","Max.","UE - IE","m","55","85","85"]
["","","System","Motsvarande","m","75","100","100"]
["","","","Ingen extra laddning","m","40","40","40"]
["","Extra köldmediemängd","","","kg/m","Se installationsmanual","Se installationsmanual","Se installationsmanual"]
["","Nivåskillnad","IU - OU","Max.","m","30.0","30.0","30.0"]
["","","IU - IU","Max.","m","0.5","0.5","0.5"]
["Standardtillbehör","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Strömförsörjning","Fas","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240"]
["Ström - 50 Hz","Max amperestyrka i säkring (MFA)","","","A","20","32","32"]
["Ljudeffektsnivå","Värme","","","dBA","","","69 (1)"]
["Anm:","","","","","","","(1) - Enligt ENER Lot 21"]