{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NV1"]
[]
[]
[]
[]
["","","","","","RZAG71N2V1B","RZAG100N7V1B","RZAG125N2V1B","RZAG140N7V1B"]
["Mått","Enhet","","Höjd","mm","870","870","870","870"]
["","","","Bredd","mm","1100","1100","1100","1100"]
["","","","Djup","mm","460","460","460","460"]
["Vikt","Enhet","","","kg","81","85","95","95"]
["Kompressor","Type","","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CTT","-20","-20","-20","-20"]
["","","","Max.","°CTT","52","52","52","52"]
["","Värme","Omgivning","Min.","°CVT","-20","-20","-20","-20"]
["","","","Max.","°CVT","18","18","18","18"]
["Ljudeffektsnivå","Kyla","","","dBA","64","66","69","70"]
["","Värme","","","dBA","","","68 (1)","71 (1)"]
["Ljudtrycksnivå","Kyla","","Nom.","dBA","46","47","49","50"]
["","Värme","","Nom.","dBA","48","50","52","52"]
["Köldmedium","Typ","","","","R-32","R-32","R-32","R-32"]
["","Mängd","","","kg","3.20","3.2","3.70","3.7"]
["","GWP","","","","675","675","675","675"]
["","Mängd","","","tCO2Eq","2.16","2.16","2.50","2.5"]
["Röranslutningar","Vätska","","YD","mm","10","10","10","10"]
["","Gas","","YD","mm","15.9","15.9","15.9","15.9"]
["","Rörledningslängd","Max.","UE - IE","m","55","85","85","85"]
["","","System","Motsvarande","m","75","100","100","100"]
["","","","Ingen extra laddning","m","40","40","40","40"]
["","Extra köldmediemängd","","","kg/m","Se installationsmanual","Se installationsmanual","Se installationsmanual","Se installationsmanual"]
["","Nivåskillnad","IU - OU","Max.","m","30","30","30","30"]
["","","IU - IU","Max.","m","0.5","0.5","0.5","0.5"]
["Standardtillbehör","Installation manual","","","","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2"]
["Strömförsörjning","Fas","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240","220-240"]
["Ström - 50 Hz","Max amperestyrka i säkring (MFA)","","","A","20","32","32","32"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor"]
["Anm:","","","","","","","(1) - Enligt ENER Lot 21","(1) - Enligt ENER Lot 21"]