{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Mått","Enhet","","Höjd","mm","1,680"]
["","","","Bredd","mm","930"]
["","","","Djup","mm","765"]
["Vikt","Enhet","","","kg","183.0"]
["Kompressor","Typ","","","","Hermetiskt försluten scrollkompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CDB","-5.0"]
["","","","Max.","°CDB","46.0"]
["","Värme","Omgivning","Min.","°CVT","-15.0"]
["","","","Max.","°CVT","15.0"]
["Ljudeffektsnivå","Kyla","","","dBA","78.0"]
["","Värme","","","dBA","78.0"]
["Köldmedium","Typ","","","","R-410A"]
["","Mängd","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Röranslutningar","Vätska","","YD","mm","9.52"]
["","Gas","","YD","mm","22.2"]
["","Rörledningslängd","Max.","UE - IE","m","100"]
["","","System","Ingen extra laddning","m","30"]
["Standardtillbehör","Installationsanvisning","","","","1"]
["","Anslutningsrör","","","","4"]
["Power supply","Fas","","","","3N~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","380-415"]
["Ström - 50Hz","Max amperestyrka i säkring (MFA)","","","A","25"]
["Anm:","","","","","(1) - Strömförsörjning för FDQ inomhusenhet är separat"]
["","","","","","(2) - Se separata ritningar för elektriska data"]
["Mått","Enhet","","Höjd","mm","","1680"]
["","","","Bredd","mm","","930"]
["","","","Djup","mm","","765"]
["Vikt","Enhet","","","kg","","184.0"]
["Kompressor","Typ","","","","","Hermetiskt försluten scrollkompressor"]
["Driftsområde","Kyla","Omgivning","Min.","°CDB","","-5.0"]
["","","","Max.","°CDB","","46.0"]
["","Värme","Omgivning","Min.","°CVT","","-15.0"]
["","","","Max.","°CVT","","15.0"]
["Ljudeffektsnivå","Kyla","","","dBA","","78.0"]
["","Värme","","","dBA","","78.0"]
["Köldmedium","Mängd","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Mängd","","","tCO2Eq","","19.4"]
["Röranslutningar","Vätska","","YD","mm","","12.70"]
["","Gas","","YD","mm","","22.2"]
["","Rörledningslängd","Max.","UE - IE","m","","100"]
["","","System","Ingen extra laddning","m","","30"]
["Standardtillbehör","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Strömförsörjning","Frequency","","","Hz","","50"]
["Ström - 50 Hz","Max amperestyrka i säkring (MFA)","","","A","","25"]