{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Ljudtrycksnivå","Värme","","Hög","dBA","","","","","","43"]
["","","","Medel","dBA","","","","","","35"]
["","","","Tyst drift","dBA","","","","","","26"]
["","","","Låg","dBA","","","","","","29"]
["","Kyla","","Medium","dBA","","","","","","34"]
["","","","Tyst drift","dBA","","","","","","20"]
["","","","Låg","dBA","","","","","","27"]
["","","","Hög","dBA","","","","","","43"]
["Standardtillbehör","Installationsanvisning","","","","","","","","","1"]
["","Bruksanvisning","","","","","","","","","1"]
["","Infraröd fjärrkontroll","","","","","","","","","1"]
["","AA torrbatterier","","","","","","","","","2"]
["","Hållare för fjärrkontroll","","","","","","","","","1"]
["","Monteringsplåt","","","","","","","","","1"]
["","Fotokatalytiskt luftreningsfilter med titanapatit","","","","","","","","","2"]
["","Fästskruvar för inomhusenhet","","","","","","","","","2"]
["Styrsystem","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Röranslutningar","Vätska","","YD","mm","","","","","","6.35"]
["","Gas","","YD","mm","","","","","","9.50"]
["","Kondensvatten","","","","","","","","","18"]
["Ineffekt","Kyla","","Nom.","kW","","","","","","0.024"]
["","Värme","","Nom.","kW","","","","","","0.029"]
["Sound power level","Kyla","","","dBA","","","","","","58"]
["","Värme","","","dBA","","","","","","58"]
["Mått","Enhet","","Bredd","mm","","","","","","770"]
["","","","Djup","mm","","","","","","225"]
["","","","Höjd","mm","","","","","","286"]
["Hölje","Färg","","","","","","","","","Vit"]
["Vikt","Enhet","","","kg","","","","","","9.0"]
["Power supply","Fas","","","","","","","","","1~"]
["","Frequency","","","Hz","","","","","","50"]
["","Namn","","","","","","","","","V1"]
["","Spänning","","","V","","","","","","220-240"]
["Anm:","","","","","","","","","","(1) - SL: Den tysta fläktnivån av luftflödeshastighetsinställningen"]
["Ineffekt","Kyla","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Värme","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Hölje","Färg","","","","Vit","Vit","Vit","Vit","Vit"]
["Mått","Enhet","","Höjd","mm","286","286","286","286","286"]
["","","","Bredd","mm","770","770","770","770","770"]
["","","","Djup","mm","225","225","225","225","225"]
["Vikt","Enhet","","","kg","8.5","8.5","8.5","8.5","9"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","","","Medel","m³/min","7.8","7.8","8","8","8.2"]
["","","","Låg","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Tyst drift","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Värme","Hög","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","","","Medel","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","","Låg","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Tyst drift","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Ljudeffektsnivå","Kyla","","","dBA","55","55","55","55","58"]
["","Värme","","","dBA","55","55","55","55","58"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","39","39","40","40","43"]
["","","","Medel","dBA","33","33","33","33","34"]
["","","","Låg","dBA","25","25","26","26","27"]
["","","","Tyst drift","dBA","20","20","20","20","20"]
["","Värme","","Hög","dBA","39","39","40","40","43"]
["","","","Medel","dBA","34","34","34","34","35"]
["","","","Låg","dBA","28","28","28","28","29"]
["","","","Tyst drift","dBA","23","23","23","23","26"]
["Röranslutningar","Vätska","","YD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","YD","mm","9.5","9.5","9.5","9.5","9.5"]
["","Kondensvatten","","","","18","18","18","18","18"]
["Styrsystem","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardtillbehör","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Strömförsörjning","Namn","","","","V1","V1","V1","V1","V1"]
["","Fas","","","","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50"]
["","Spänning","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standardtillbehör","AAA dry-cell batteries","","","","","2","","2","2"]
["Styrsystem","Infraröd fjärrkontroll","","","","","","ARC480A11","ARC480A11"]
["Standardtillbehör","Titanium apatite photocatalytic air purification filter","","","","","","2"]