{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF42C5V1B","ATXF35C5V1B (Archived)"]
["Ljudtrycksnivå","Värme","","Hög","dBA","39.0","40.0","44.0"]
["","","","Medel","dBA","34.0","34.0","34.0"]
["","","","Tyst drift","dBA","21.0","21.0","22.0"]
["","","","Låg","dBA","28.0","28.0","28.0"]
["","Kyla","","Medel","dBA","33.0","33.0","36.0"]
["","","","Tyst drift","dBA","20.0","20.0","22.0"]
["","","","Låg","dBA","25.0","26.0","30.0"]
["","","","Hög","dBA","39.0","40.0","45.0"]
["Standardtillbehör","Installationsanvisning","","","","1","1","1"]
["","Bruksanvisning","","","","1","1","1"]
["","Batterier","","","","1","1","1"]
["","Infraröd fjärrkontroll","","","","1","1","1"]
["","AAA torrbatterier","","","","2","2","2"]
["","Hållare för fjärrkontroll","","","","1","1","1"]
["","Monteringsplåt","","","","1","1","1"]
["","Fästskruvar för inomhusenhet","","","","2","2","2"]
["Styrsystem","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["Piping connections","Vätska","","YD","mm","6.35","6.35","6.35"]
["","Gas","","YD","mm","9.50","9.50","9.50"]
["","Drain","","","","18","18","18"]
["Effektförbrukning","Kyla","","Nom.","kW","0.023","0.023","0.040"]
["","Värme","","Nom.","kW","0.023","0.023","0.040"]
["Ljudeffektsnivå","Kyla","","","dBA","53.0","54.0","59.0"]
["","Värme","","","dBA","55.0","55.0","59.0"]
["Mått","Enhets-","","Bredd","mm","770","770","770"]
["","","","Djup","mm","225","225","225"]
["","","","Höjd","mm","286","286","286"]
["Hölje","Colour","","","","Vit","Vit","Vit"]
["Vikt","Enhet","","","kg","8.00","8.00","9.00"]
["Power supply","Fas","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Spänning","","","V","220-440","220-440","220-440"]
["Ineffekt","Kyla","","Nom.","kW","","","","0.029"]
["","Värme","","Nom.","kW","","","","0.029"]
["Hölje","Färg","","","","","","","Vit"]
["Mått","Enhet","","Höjd","mm","","","","286"]
["","","","Bredd","mm","","","","770"]
["","","","Djup","mm","","","","225"]
["Vikt","Enhet","","","kg","","","","8.5"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","","","","11.8"]
["","","","Medel","m³/min","","","","8"]
["","","","Låg","m³/min","","","","6.4"]
["","","","Tyst drift","m³/min","","","","4.4"]
["","","Värme","Hög","m³/min","","","","11.9"]
["","","","Medel","m³/min","","","","8.6"]
["","","","Låg","m³/min","","","","6.5"]
["","","","Tyst drift","m³/min","","","","5.3"]
["Ljudeffektsnivå","Kyla","","","dBA","","","","54"]
["","Värme","","","dBA","","","","56"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","","","43"]
["","","","Medel","dBA","","","","34"]
["","","","Låg","dBA","","","","27"]
["","","","Tyst drift","dBA","","","","20"]
["","Värme","","Hög","dBA","","","","40"]
["","","","Medel","dBA","","","","35"]
["","","","Låg","dBA","","","","29"]
["","","","Tyst drift","dBA","","","","21"]
["Röranslutningar","Vätska","","YD","mm","","","","6.35"]
["","Gas","","YD","mm","","","","9.5"]
["","Kondensvatten","","","","","","","18"]
["Styrsystem","Infraröd fjärrkontroll","","","","","","","ARC470A1"]
["","Kabelansluten fjärrkontroll","","","","","","","BRC073A1"]
["Standardtillbehör","Installation manual","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","Operation manual","","","","","","","1"]
["","Batteries","","","","","","","1"]
["","Indoor unit fixing screws","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Mounting plate","","","","","","","1"]
["","Remote control holder","","","","","","","1"]
["Strömförsörjning","Fas","","","","","","","1~"]
["","Frequency","","","Hz","","","","50"]
["","Spänning","","","V","","","","220-440"]