{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B","ATXM20R5V1B","ATXM25R2V1B","ATXM25R5V1B","ATXM35R2V1B","ATXM35R5V1B","ATXM50R2V1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","39"]
["","","","Medel","dBA","34"]
["","","","Tyst drift","dBA","20"]
["","","","Låg","dBA","26"]
["","Kyla","","Medel","dBA","33"]
["","","","Tyst drift","dBA","19"]
["","","","Låg","dBA","25"]
["","","","Hög","dBA","41"]
["Standardtillbehör","Installationsanvisning","","","","1"]
["","Bruksanvisning","","","","1"]
["","Trådlös fjärrkontroll","","","","1"]
["","AAA torrbatterier","","","","2"]
["","Hållare för fjärrkontroll","","","","1"]
["","Monteringsplåt","","","","1"]
["","Luftreningsfilter med titanapatit","","","","1"]
["","Fästskruvar för inomhusenhet","","","","2"]
["","Adaptersats för WLAN","","","","1"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Röranslutningar","Vätska","","YD","mm","6.35"]
["","Gas","","YD","mm","9.50"]
["","Kondensvatten","","","","18"]
["Ineffekt","Kyla","","Nom.","kW","0.029"]
["","Värme","","Nom.","kW","0.023"]
["Ljudeffektsnivå","Kyla","","","dBA","58"]
["","Värme","","","dBA","55"]
["Mått","Enhet","","Bredd","mm","778"]
["","","","Djup","mm","272"]
["","","","Höjd","mm","295"]
["Hölje","Färg","","","","Vit"]
["Vikt","Enhet","","","kg","10.0"]
["Fläkt","Luftflödeshastighet","Värme","Hög","m³/min","9.3"]
["","","","Medel","m³/min","8.2"]
["","","","Låg","m³/min","6.2"]
["","","","Tyst drift","m³/min","5.1"]
["","","Kyla","Låg","m³/min","5.7"]
["","","","Medel","m³/min","7.5"]
["","","","Hög","m³/min","10.5"]
["","","","Tyst drift","m³/min","4.3"]
["Power supply","Fas","","","","1~"]
["","Namn","","","","V1"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]
["Anm:","","","","","(1) - Kyla: inomhustemperatur. 27 °CTT, 19,0 °CVT, utomhustemperatur. 35 °CTT, 24 °CVT, ekvivalent rörledningslängd: 5 m"]
["","","","","","(2) - Värme: inomhustemperatur. 20 °CTT; utomhustemperatur 7°CTT, 6°CVT; ekvivalent köldmedierörledning: 5m"]
["Ineffekt","Kyla","","Nom.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Värme","","Nom.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Hölje","Färg","","","","","Vit","Vit","Vit","Vit","Vit","Vit","Vit"]
["Mått","Enhet","","Höjd","mm","","295","295","295","295","295","295","299"]
["","","","Bredd","mm","","778","778","778","778","778","778","998"]
["","","","Djup","mm","","272","272","272","272","272","272","292"]
["Vikt","Enhet","","","kg","","10","10","10","10","10","10","14.5"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","","","Medel","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","Låg","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Tyst drift","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Värme","Hög","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","","","Medel","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","","Låg","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Tyst drift","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Ljudeffektsnivå","Kyla","","","dBA","","58","58","58","58","58","58","58"]
["","Värme","","","dBA","","55","55","55","55","55","55","58"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","41","41","41","41","45","45","44"]
["","","","Medel","dBA","","33","33","33","33","33","33","40"]
["","","","Låg","dBA","","25","25","25","25","25","25","36"]
["","","","Tyst drift","dBA","","19","19","19","19","19","19","27"]
["","Värme","","Hög","dBA","","39","39","39","39","39","39","43"]
["","","","Medel","dBA","","34","34","34","34","35","35","39"]
["","","","Låg","dBA","","26","26","27","27","28","28","34"]
["","","","Tyst drift","dBA","","20","20","20","20","20","20","31"]
["Röranslutningar","Vätska","","YD","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","YD","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Kondensvatten","","","","","18","18","18","18","18","18","18"]
["Styrsystem","Infrared remote control","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardtillbehör","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Strömförsörjning","Namn","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Fas","","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","","50","50","50","50","50","50","50"]
["","Spänning","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardtillbehör","Silver particle filter","","","","","","","","","","","1"]