{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53B"]
[]
[]
[]
[]
["","","","","BRC1E53B7"]
["Emballage","Material","","","Kartong_"]
["","Vikt","","kg","0.05"]
["Omgivningstemperatur","Relativ luftfuktighet <","","%","95"]
["Mått","Paketerad enhet","Bredd","mm","160"]
["","","Höjd","mm","55"]
["","","Djup","mm","150"]
["","Enhet","Bredd","mm","120"]
["","","Djup","mm","19"]
["","","Höjd","mm","120"]
["Hölje","Knappskydd","","","nej"]
["","Färg","","","Fräscht vit"]
["","Drift-LED","Färg","","Grön"]
["LCD","Typ","","","Full punkt (160 x 255)"]
["","Bakgrundsbelysning","Färg","","Vit"]
["","Dimensioner","Bredd","mm","68.85"]
["","","Höjd","mm","43.2"]
["Vikt","Paketerad enhet","","kg","0.415"]
["","Enhet","","kg","0.200"]
["Backup för strömavbrott","","","","Ja (klockan fortsätter fungera i en tid som inte överskrider 48 timmar)"]
["Ledningsdragningsanslutningar","Ledningsdragningslängd","Max.","m","500"]