{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H519W"]
[]
[]
[]
[]
["","","","","BRC1H519W."]
["Emballage","Material","","","Kartong"]
["","Vikt","","kg","0.0850"]
["Omgivningstemperatur","Relativ luftfuktighet <","","%","95"]
["Mått","Paketerad enhet","Bredd","mm","217"]
["","","Höjd","mm","50"]
["","","Djup","mm","161"]
["","Enhet","Bredd","mm","85"]
["","","Djup","mm","25"]
["","","Höjd","mm","85"]
["Hölje","Knappskydd","","","nej"]
["","Färg","","","Vit"]
["","Drift-LED","Färg","","Blue status indicator"]
["LCD","Typ","","","100 x 150 dots"]
["","Bakgrundsbelysning","Färg","","Vit"]
["","Dimensioner","Bredd","mm","28.0"]
["","","Höjd","mm","40.7"]
["Vikt","Paketerad enhet","","kg","0.317"]
["","Enhet","","kg","0.110"]
["Ledningsdragningsanslutningar","Ledningsdragningslängd","Max.","m","500"]