{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BB"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BB"]
["Ljudtrycksnivå","Värme","","Hög","dBA","39"]
["","","","Medel","dBA","32"]
["","","","Tyst drift","dBA","21"]
["","","","Låg","dBA","25"]
["","Kyla","","Medel","dBA","32"]
["","","","Tyst drift","dBA","21"]
["","","","Låg","dBA","25"]
["","","","Hög","dBA","39"]
["Standardtillbehör","Installationsanvisning","","","","1"]
["","Bruksanvisning","","","","1"]
["","Luftfilter","","","","2"]
["","Infraröd fjärrkontroll","","","","1"]
["","Fjärrkontrollens monteringsplåt","","","","1"]
["","Skruvpåse","","","","1"]
["","Skruvlock","","","","2"]
["","AAA torrbatterier","","","","2"]
["","Allmänna säkerhetsföreskrifter","","","","1"]
["Köldmedium","GWP","","","","675.0"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Röranslutningar","Vätska","","YD","mm","6.35"]
["","Gas","","YD","mm","9.50"]
["","Kondensvatten","","","","18"]
["Ineffekt","Kyla","","Nom.","kW","0.020"]
["","Värme","","Nom.","kW","0.020"]
["Ljudeffektsnivå","Kyla","","","dBA","57"]
["Mått","Enhet","","Bredd","mm","798"]
["","","","Djup","mm","189"]
["","","","Höjd","mm","295"]
["Hölje","Färg","","","","Svart"]
["Vikt","Enhet","","","kg","11.5"]
["Fläkt","Luftflödeshastighet","Värme","Hög","m³/min","10.9"]
["","","","Medel","m³/min","8.7"]
["","","","Låg","m³/min","6.4"]
["","","","Tyst drift","m³/min","4.5"]
["","","Kyla","Låg","m³/min","6.1"]
["","","","Medel","m³/min","8.2"]
["","","","Hög","m³/min","11.0"]
["","","","Tyst drift","m³/min","4.6"]
["Power supply","Fas","","","","1~"]
["","Namn","","","","V1"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]