{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Ljudtrycksnivå","Värme","","Hög","dBA","38","","41"]
["","","","Tyst drift","dBA","21","","21"]
["","","","Låg","dBA","28","","30"]
["","Kyla","","Tyst drift","dBA","21","","21"]
["","","","Låg","dBA","25","","28"]
["","","","Hög","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Kyla","","Nom.","dBA","31","","35"]
["Standardtillbehör","Installationsanvisning","","","","1","","1"]
["","Bruksanvisning","","","","1","","1"]
["","Trådlös fjärrkontroll","","","","1","","1"]
["","Batterier","","","","2","","2"]
["","Hållare för fjärrkontroll","","","","1","","1"]
["","Monteringsplåt","","","","1","","1"]
["","Fästskruvar för inomhusenhet","","","","2","","2"]
["","Fotokatalytiskt luftreningsfilter med titanapatit","","","","2","","2"]
["Styrsystem","Infraröd fjärrkontroll","","","","ARC466A6","","ARC466A6"]
["Piping connections","Vätska","","YD","mm","6.35","","6.35"]
["","Gas","","YD","mm","9.5","","9.5"]
["","Kondensvatten","","","","18","","18"]
["Ineffekt","Kyla","","Nom.","kW","0.040","","0.040"]
["","Värme","","Nom.","kW","0.040","","0.040"]
["Sound power level","Kyla","","","dBA","55","","59"]
["","Värme","","","dBA","56","","58"]
["Mått","Enhet","","Bredd","mm","780","","780"]
["","","","Djup","mm","215","","215"]
["","","","Höjd","mm","289","","289"]
["Hölje","Colour","","","","Vit","","Vit"]
["Vikt","Enhet","","","kg","8","","8"]
["Fläkt","Luftflödeshastighet","Värme","Hög","m³/min","","","10.1"]
["","","","Låg","m³/min","","","6.3"]
["","","","Tyst drift","m³/min","","","4.3"]
["","","Kyla","Låg","m³/min","","","5.2"]
["","","","Hög","m³/min","","","9.2"]
["","","","Tyst drift","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Kyla","Nom.","m³/min","","","7.2"]
["Power supply","Fas","","","","1~","","1~"]
["","Frequency","","","Hz","50","","50"]
["","Namn","","","","V1","","V1"]
["","Spänning","","","V","220-240","","220-240"]
["Anm:","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Ineffekt","Kyla","","Nom.","kW","","0.04","","0.040"]
["","Värme","","Nom.","kW","","0.04","","0.040"]
["Hölje","Färg","","","","","Vit","","Vit"]
["Mått","Enhet","","Höjd","mm","","289","","289"]
["","","","Bredd","mm","","780","","780"]
["","","","Djup","mm","","215","","215"]
["Vikt","Enhet","","","kg","","8","","8.00"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","","7.9","","9.2"]
["","","","Medel","m³/min","","6.3","","7.2"]
["","","","Låg","m³/min","","4.7","","5.2"]
["","","","Tyst drift","m³/min","","3.9","","3.9"]
["","","Värme","Hög","m³/min","","9","","10.1"]
["","","","Medel","m³/min","","7.5","","8.1"]
["","","","Låg","m³/min","","6","","6.3"]
["","","","Tyst drift","m³/min","","4.3","","4.3"]
["Ljudeffektsnivå","Kyla","","","dBA","","55","","59"]
["","Värme","","","dBA","","56","","58"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","37","","42"]
["","","","Medel","dBA","","31","","35"]
["","","","Låg","dBA","","25","","28"]
["","","","Tyst drift","dBA","","21","","21"]
["","Värme","","Hög","dBA","","38","","41"]
["","","","Medel","dBA","","33","","36"]
["","","","Låg","dBA","","28","","30"]
["","","","Tyst drift","dBA","","21","","21"]
["Röranslutningar","Vätska","","YD","mm","","6.35","","6.35"]
["","Gas","","YD","mm","","9.5","","9.50"]
["","Kondensvatten","","","","","18","","18"]
["Styrsystem","Infraröd fjärrkontroll","","","","","ARC466A6","","ARC466A6"]
["Standardtillbehör","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Strömförsörjning","Namn","","","","","V1","","V1"]
["","Fas","","","","","1~","","1~"]
["","Frequency","","","Hz","","50","","50"]
["","Spänning","","","V","","220-240","","220-240"]