{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","E1500"]
[]
[]
[]
[]
["","","","","EZESHP20AUAW1B"]
["Kylkapacitet","Vid börvärde 0 °C (30 °C omgivningstemperatur)","R-452A","kW","14,900"]
["","Vid börvärde -20 °C (30 °C omgivningstemperatur)","R-452A","kW","9,200"]
["Uppvärmningseffekt","Vid börvärde +2 °C (-20 °C omgivningstemperatur)","R-452A","kW","10,500"]
["Ineffekt","Motor","Type","","Kubota Custom Diesel Engine, 4 Cylinders, NRMM Stage V Compliant"]
["","","Förskjutning","cc","1,500"]
["","","Underhållsintervall","hr","3,000"]
["","Generator","Type","","Direct Drive"]
["","","Effekt","kW","15"]
["Mått","Enhet","Höjd","mm","2,227"]
["","","Bredd","mm","2,072"]
["","","Djup","mm","440"]
["","Paketerad enhet","Höjd","mm","2,066"]
["","","Bredd","mm","2,345"]
["","","Djup","mm","542"]
["Vikt","Enhet","","kg","730"]
["Kompressor","Typ","","","Custom Scroll Compressor - Economizer/Inverter"]
["Köldmedium","Typ","","","R-452A"]
["Ljudtrycksnivå","Nom.","","dBA","65"]
["Power supply","Spänning","","V","400"]
["","Fas","","","3P+N"]
["","Frequency","","Hz","50"]