{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":17,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-E6V / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHVH04S18EA6V / ERGA04EAV3A","EHVH04S18EJ6V / ERGA04EAV3A","EHVH04S23EA6V / ERGA04EAV3A","EHVH04S23EJ6V / ERGA04EAV3A","EHVH08S18EA6V / ERGA06EAV3A","EHVH08S18EJ6V / ERGA06EAV3A","EHVH08S23EA6V / ERGA06EAV3A","EHVH08S23EJ6V / ERGA06EAV3A","EHVH08S18EA6V / ERGA08EAV3A","EHVH08S18EJ6V / ERGA08EAV3A","EHVH08S23EA6V / ERGA08EAV3A","EHVH08S23EJ6V / ERGA08EAV3A"]
["Värmekapacitet","Nom.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Ineffekt","Värme","","Nom.","kW","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["Effektförbrukning","Varmvatten från 10°C till 50°C","","Nom.","kWh","2.48","2.48","3.01","3.01","2.48","2.48","3.01","3.01","2.48","2.48","3.01","3.01"]
["Uppvärmning från 10°C till 50°C","hr","","","","1h28min","1h28min","1h40min","1h40min","1h28min","1h28min","1h40min","1h40min","1h28min","1h28min","1h40min","1h40min"]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Tappvattenvärmning","Allmänt","","Deklarerad belastningsprofil","","L","L","XL","XL","L","L","XL","XL","L","L","XL","XL"]
["","Medelklimat","","Energieffektivitetsklass för vattenuppvärmning","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","SCOP","","3.26","3.26","3.26","3.26","3.25","3.25","3.25","3.25","3.27","3.27","3.27","3.27"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Framledningstemperatur vid medelklimat 35°C","Allmänt","SCOP","","4.48","4.48","4.48","4.48","4.47","4.47","4.47","4.47","4.56","4.56","4.56","4.56"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Intervall för energieffektivitet","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Anm:","","","","","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Tillstånd 1: kyla Ta 35 °C - LWE 18 °C (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Tillstånd 2: kyla Ta 35 °C - LWE 7℃ (DT = 5 °C); värme Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]