{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPBX10A4V / EPSK08-10AW1"]
[]
[]
[]
[]
["","","","","","EPBX10AF4V / EPSK08ARW1","EPBX10AF4V / EPSK10ARW1"]
["Inomhusdel","","","","","EPBX10AF4V","EPBX10AF4V"]
["Värmekapacitet","Nom.","","","kW","7.62 (1)","8.11 (1)"]
["Kylkapacitet","Nom.","","","kW","6.89 (2), 6.37 (3)","7.84 (2), 6.37 (3)"]
["Ineffekt","Värme","","Nom.","kW","1.52 (1)","1.64 (1)"]
["","Kyla","","Nom.","kW","1.85 (2), 1.13 (3)","2.17 (2), 1.13 (3)"]
["COP","","","","","5.01 (1)","4.94 (1)"]
["EER","","","","","3.73 (2), 5.63 (3)","3.62 (2), 5.63 (3)"]
["Rumsuppvärmning","Framledningstemperatur vid medelklimat 55°C","Allmänt","SCOP","","3.94","3.99"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A+++","A+++"]
["","Framledningstemperatur vid medelklimat 35°C","Allmänt","SCOP","","5.14","5.14"]
["","","","Klass för årstidsrelaterad verkningsgrad","","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Anm:","","","","","(1) - Förhållande: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Förhållande: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Kyla: EW 12°C; LW 7°C; omgivningsförhållanden: 35 °CTT","(2) - Kyla: EW 12°C; LW 7°C; omgivningsförhållanden: 35 °CTT"]
["","","","","","(3) - Kyla: EW 23°C; LW 18°C; omgivningsförhållanden: 35 °CTT","(3) - Kyla: EW 23°C; LW 18°C; omgivningsförhållanden: 35 °CTT"]