{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSX10A"]
[]
[]
[]
[]
["","","","","","EPSX10P30AF","EPSX10P50AF"]
["Hölje","Färg","","","","Trafikvit (RAL9016), Grafitsvart (RAL9011), Kolsvart (RAL9005)","Trafikvit (RAL9016), Grafitsvart (RAL9011), Kolsvart (RAL9005)"]
["","Material","","","","Stryktålig polypropylen","Stryktålig polypropylen"]
["Mått","Enhet","","Höjd","mm","1914","1906"]
["","","","Bredd","mm","590","785"]
["","","","Djup","mm","671","837"]
["Vikt","Enhet","","","kg","84.0","105"]
["PED","Kategori","","","","Art 4.3","Art 4.3"]
["Ljudeffektsnivå","Nom.","","","dBA","49.0","49.0"]
["Ljudtrycksnivå","Nom.","","","dBA","35.0","35.0"]
["Driftsområde","Värme","Vattensida","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["","Kyla","Omgivning","Min.","°CTT","0 (3)","0 (3)"]
["","","Vattensida","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["Strömförsörjning","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","230","230"]
["Elektrisk värmare","Strömförsörjning","","Namn","","6V / 9W","6V / 9W"]
["","","","Fas","","1~ / 3~","1~ / 3~"]
["","","","Frequency","Hz","50","50"]
["","","","Spänning","V","230/400","230/400"]
["Elvärmare","Rekommenderade säkringar","","","A","0 (4)","0 (4)"]
["Anm:","","","","","(1) - Värmeförlust enligt EN12897","(1) - Värmeförlust enligt EN12897"]
["","","","","","(2) - Minsta erforderliga volym, exklusive volymen i enheten","(2) - Minsta erforderliga volym, exklusive volymen i enheten"]
["","","","","","(3) - Se ritning för driftgränser","(3) - Se ritning för driftgränser"]
["","","","","","(4) - Se kopplingsschemat och installationsmanualen för korrekt rekommenderad säkring beroende på strömförsörjning och nätanslutning","(4) - Se kopplingsschemat och installationsmanualen för korrekt rekommenderad säkring beroende på strömförsörjning och nätanslutning"]