{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Ljudtrycksnivå","Värme","","Hög","dBA","35.0","35.0"]
["","","","Låg","dBA","29.0","29.0"]
["","Kyla","","Låg","dBA","28.0","28.0"]
["","","","Hög","dBA","35.0","35.0"]
["Standardtillbehör","Installations- och bruksanvisning","","","","1","1"]
["","Sugluftfilter","","","","1","1"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","BRC1D52, BRC1E52A/B"]
["Röranslutningar","Vätska","","YD","mm","6.35"]
["","Gas","","YD","mm","9.52"]
["","Drain","","","","27.2"]
["Sound power level","Kyla","","","dBA","55","55"]
["","Värme","","","dBA","55","55"]
["Mått","Enhet","","Bredd","mm","652","652"]
["","","","Djup","mm","502","502"]
["","","","Höjd","mm","230","230"]
["Hölje","Material","","","","Förzinkat stål","Förzinkat stål"]
["Vikt","Enhet","","","kg","17.0","17.0"]
["Fläkt","Luftflödeshastighet","Värme","Hög","m³/min","","6.95"]
["","","","Låg","m³/min","","5.20"]
["","","Kyla","Låg","m³/min","","5.20"]
["","","","Hög","m³/min","","6.50"]
["Power supply","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Namn","","","","V1","V1"]
["","Spänning","","","V","230","230 +/-10%"]
["Anm:","","","","","(1) - Ljudvärdena är uppmätta i ett semi-ekofritt rum.","(1) - Ljudvärdena är uppmätta i ett semi-ekofritt rum."]
["","","","","","(2) - Ljudtrycksnivån ett relativt värde som beror på avståndet och den omgivande akustiken. För mer information, läs ljudnivåritningarna.","(2) - Ljudtrycksnivån ett relativt värde som beror på avståndet och den omgivande akustiken. För mer information, läs ljudnivåritningarna."]
["","","","","","(3) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar.","(3) - Ljudeffektsnivån är ett absolut värde som anger vilken effekt en ljudkälla genererar."]
["Röranslutningar","Vätska","","YD","mm","","6.35"]
["","Gas","","YD","mm","","9.52"]
["","Drain","","","","","27.2"]