{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Ljudtrycksnivå","Värme","","Hög","dBA","35.0","35.0","","38.0"]
["","","","Medel","dBA","33.0","33.0","","35.0"]
["","","","Låg","dBA","27.0","27.0","","30.0"]
["","Kyla","","Medel","dBA","33.0","33.0","","35.0"]
["","","","Låg","dBA","27.0","27.0","","30.0"]
["","","","Hög","dBA","35.0","35.0","","38.0"]
["Standardtillbehör","Installationsanvisning","","","","1","1","","1"]
["","Bruksanvisning","","","","1","1","","1"]
["","Isolering för anslutningsdel","","","","1","1","","1"]
["","Tätningsbelägg","","","","1","1","","1"]
["","Metall för rörhållare","","","","1","1","","1"]
["","Kondensvattenslang","","","","1","1","","1"]
["","Bricka för hängarfäste","","","","8","8","","8"]
["","Tätningsmaterial","","","","2","2","","2"]
["","Rörhållare","","","","6","6","","6"]
["","Brickhållarplåt","","","","4","4","","4"]
["","Skruvar för rörflänsar","","","","1","1","","1"]
["","Luftfilter","","","","1","1","","1"]
["Röranslutningar","Vätska","","YD","mm","6.35","6.35","","6.35"]
["","Gas","","YD","mm","9.50","9.50","","12.70"]
["","Kondensvatten","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Ineffekt","Kyla","","Nom.","kW","0.036","0.036","","0.060"]
["","Värme","","Nom.","kW","0.036","0.036","","0.060"]
["Ljudeffektsnivå","Kyla","","","dBA","53.0","53.0","","56.0"]
["","Värme","","","dBA","53.0","53.0","","56.0"]
["Mått","Enhet","","Bredd","mm","750","750","","1,150"]
["","","","Djup","mm","620","620","","620"]
["","","","Höjd","mm","200","200","","200"]
["Vikt","Enhet","","","kg","21","21","","28"]
["Fläkt","Yttre statiskt tryck","","Nom.","Pa","30","30","","40"]
["","Luftflödeshastighet","Värme","Hög","m³/min","8.7","8.7","","16.0"]
["","","","Medel","m³/min","8.0","8.0","","14.8"]
["","","","Låg","m³/min","7.3","7.3","","13.5"]
["","","Kyla","Låg","m³/min","7.3","7.3","","13.5"]
["","","","Medel","m³/min","8.0","8.0","","14.8"]
["","","","Hög","m³/min","8.7","8.7","","16.0"]
["Power supply","Fas","","","","1~","1~","","1~"]
["","Frequency","","","Hz","50","50","","50"]
["","Spänning","","","V","220-240","220-240","","220-240"]
["Anm:","","","","","(1) - Se separata ritningar för elektriska data","(1) - Se separata ritningar för elektriska data","","(1) - Se separata ritningar för elektriska data"]
["Ineffekt","Kyla","","Nom.","kW","","","0.060"]
["","Värme","","Nom.","kW","","","0.060"]
["Mått","Enhet","","Höjd","mm","","","200"]
["","","","Bredd","mm","","","1150"]
["","","","Djup","mm","","","620"]
["Vikt","Enhet","","","kg","","","28"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","","","15.8"]
["","","","Medel","m³/min","","","14.6"]
["","","","Låg","m³/min","","","13.3"]
["","","Värme","Hög","m³/min","","","15.8"]
["","","","Medel","m³/min","","","14.6"]
["","","","Låg","m³/min","","","13.3"]
["","Yttre statiskt tryck","","Nom.","Pa","","","40"]
["Ljudeffektsnivå","Kyla","","","dBA","","","55.0"]
["","Värme","","","dBA","","","55.0"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","","","38.0"]
["","","","Medel","dBA","","","35.0"]
["","","","Låg","dBA","","","30.0"]
["","Värme","","Hög","dBA","","","38.0"]
["","","","Medel","dBA","","","35.0"]
["","","","Låg","dBA","","","30.0"]
["Röranslutningar","Vätska","","YD","mm","","","6.35"]
["","Gas","","YD","mm","","","12.70"]
["","Kondensvatten","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standardtillbehör","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Luftfilter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Strömförsörjning","Fas","","","","","","1~"]
["","Frequency","","","Hz","","","50"]
["","Spänning","","","V","","","220-240"]