{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Ljudtrycksnivå","Värme","Hög","dBA","46"]
["","","Tyst drift","dBA","30"]
["","","Låg","dBA","33"]
["","Kyla","Tyst drift","dBA","29"]
["","","Låg","dBA","32"]
["","","Hög","dBA","38"]
["","","Nom.","dBA","36"]
["","Kyla","Nom.","dBA","35"]
["Standardtillbehör","Installationsanvisning","","","1"]
["","Bruksanvisning","","","1"]
["","Infraröd fjärrkontroll","","","1"]
["","AAA torrbatterier","","","2"]
["","Hållare för fjärrkontroll","","","1"]
["","Monteringsplåt","","","1"]
["","Värmeisoleringsrör (rörledning för köldmedie)","","","8"]
["","Luftreningsfilter","","","1"]
["","Fotokatalytiskt luktreducerande filter","","","1"]
["","Sidokåpa","","","2"]
["","Bindningsband","","","4"]
["Styrsystem","Infrared remote control","","","ARC433B67"]
["Röranslutningar","Vätska","YD","mm","6.35"]
["","Gas","YD","mm","9.5"]
["","Kondensvatten","","","18"]
["Ljudeffektsnivå","Kyla","","dBA","53"]
["","Värme","","dBA","59"]
["Mått","Enhet","Bredd","mm","1,050"]
["","","Djup","mm","200"]
["","","Höjd","mm","490"]
["Hölje","Colour","","","Mandelvit"]
["Vikt","Enhet","","kg","16"]
["Power supply","Phase","","","1~"]
["","Frequency","","Hz","50"]
["","Namn","","","VM"]
["","Spänning","","V","220-240"]
["Anm:","","","","(1) - 220V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]
["","","","","(4) - Vid anslutning till en utomhusdel med multisystem, se specifikationerna för multiutomhusdelen som ska anslutas."]