{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CB"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BB"]
["Ineffekt","Kyla","","Nom.","kW","0.023"]
["","Värme","","Nom.","kW","0.022"]
["Hölje","Färg","","","","Svart"]
["Mått","Enhet","","Höjd","mm","295"]
["","","","Bredd","mm","798"]
["","","","Djup","mm","189"]
["Vikt","Enhet","","","kg","12"]
["Fläkt","Luftflödeshastighet","Kyla","Hög","m³/min","13.1"]
["","","","Medel","m³/min","9"]
["","","","Låg","m³/min","6"]
["","","","Tyst drift","m³/min","4.9"]
["","","Värme","Hög","m³/min","12.3"]
["","","","Medel","m³/min","8.2"]
["","","","Låg","m³/min","5.8"]
["","","","Tyst drift","m³/min","5"]
["Ljudeffektsnivå","Kyla","","","dBA","60"]
["","Värme","","","dBA","60"]
["Ljudtrycksnivå","Kyla","","Hög","dBA","43"]
["","","","Medel","dBA","32"]
["","","","Låg","dBA","25"]
["","","","Tyst drift","dBA","20"]
["","Värme","","Hög","dBA","41"]
["","","","Medel","dBA","31"]
["","","","Låg","dBA","24"]
["","","","Tyst drift","dBA","19"]
["Köldmedium","GWP","","","","675"]
["Röranslutningar","Vätska","","YD","mm","6.35"]
["","Gas","","YD","mm","9.5"]
["","Kondensvatten","","","","18"]
["Styrsystem","Infrared remote control","","","","ARC466A84"]
["Styrsystem","Kabelansluten fjärrkontroll","","","","BRC073A4"]
["Standardtillbehör","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Strömförsörjning","Fas","","","","1~"]
["","Frequency","","","Hz","50"]
["","Spänning","","","V","220-240"]