{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Ljudtrycksnivå","Värme","Hög","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["","","Låg","dBA","38","44","46","48"]
["","Kyla","Låg","dBA","38","44","46","48"]
["","","Hög","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["Standardtillbehör","Bruksanvisning","","","Bruksanvisning","Bruksanvisning","Bruksanvisning","Bruksanvisning"]
["","Installationsanvisning","","","Installationsanvisning","Installationsanvisning","Installationsanvisning","Installationsanvisning"]
["","Konsol för installation","","","Konsol för installation","Konsol för installation","Konsol för installation","Konsol för installation"]
["","Skyddsgummi för hål","","","Skyddsgummi för hål","Skyddsgummi för hål","Skyddsgummi för hål","Skyddsgummi för hål"]
["","Bussning","","","Bussning","Bussning","Bussning","Bussning"]
["","Isolering för anslutningsdel","","","Isolering för anslutningsdel","Isolering för anslutningsdel","Isolering för anslutningsdel","Isolering för anslutningsdel"]
["","Lock","","","Lock","Lock","Lock","Lock"]
["","Rörhållare","","","Rörhållare","Rörhållare","Rörhållare","Rörhållare"]
["","Skruvar","","","Skruvar","Skruvar","Skruvar","Skruvar"]
["","Installationsmönster","","","Installationsmönster","Installationsmönster","Installationsmönster","Installationsmönster"]
["","Daggskyddat material","","","Daggskyddat material","Daggskyddat material","Daggskyddat material","Daggskyddat material"]
["","Kabel till fjärrkontroll","","","Kabel till fjärrkontroll","Kabel till fjärrkontroll","Kabel till fjärrkontroll","Kabel till fjärrkontroll"]
["Styrsystem","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Röranslutningar","Vätska","YD","mm","9.52","9.52","9.52","9.52"]
["","Gas","YD","mm","15.9","15.9","15.9","15.9"]
["","Kondensvatten","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Ineffekt","Kyla","Nom.","kW","0.117","0.238","0.238","0.276"]
["","Värme","Nom.","kW","0.117","0.238","0.238","0.276"]
["Ljudeffektsnivå","Kyla","","dBA","55","62","63","65"]
["","Värme","","dBA","55","62","63","65"]
["Mått","Enhet","Bredd","mm","600","600","600","600"]
["","","Djup","mm","270","350","350","350"]
["","","Höjd","mm","1,850","1,850","1,850","1,850"]
["Hölje","Färg","","","Fräscht vit","Fräscht vit","Fräscht vit","Fräscht vit"]
["Vikt","Enhet","","kg","39","47","47","47"]
["Power supply","Fas","","","1~","1~","1~","1~"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60"]
["","Spänning","","V","220-240/220","220-240/220","220-240/220","220-240/220"]