{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N9"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B9","RXTP35N2V1B9"]
["Ljudtrycksnivå","Värme","","Nom.","dBA","49","49"]
["","Kyla","","Nom.","dBA","48","48"]
["Standardtillbehör","Installationsanvisning","","","","1","1"]
["","Etikett för köldmediemängd","","","","1","1"]
["","Flerspråkiga etiketter om fluorerande växthusgas","","","","1","1"]
["Köldmedium","Charge","","","TCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["","Mängd","","","kg","1.1","1.1"]
["","Typ","","","","R-32","R-32"]
["Fläktmotor","Hastighet","Kyla","Superlåg","varv/min","450","450"]
["","","Värme","Superlåg","varv/min","360","360"]
["Driftsområde","Kyla","Omgivning","Max.","°CTT","46","46"]
["","","","Min.","°CTT","-10","-10"]
["","Värme","Omgivning","Max.","°CVT","18","18"]
["","","","Min.","°CVT","-25","-25"]
["Röranslutningar","Nivåskillnad","IU - OU","Max.","m","15","15"]
["","Extra köldmediemängd","","","kg/m","0,02 (för rördragning över 10m)","0,02 (för rördragning över 10m)"]
["Kompressor","Typ","","","","Hermetiskt tillsluten swing-kompressor","Hermetiskt tillsluten swing-kompressor"]
["Mått","Enhet","","Bredd","mm","763","763"]
["","","","Djup","mm","312","312"]
["","","","Höjd","mm","551","551"]
["Vikt","Enhet","","","kg","38","38"]
["Power supply","Fas","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Spänning","","","V","220-240","220-240"]
["Anm:","","","","","(1) - Innehåller fluorerande växthusgas","(1) - Innehåller fluorerande växthusgas"]
["","","","","","(2) - Se separat ritning för driftsområde","(2) - Se separat ritning för driftsområde"]
["","","","","","(3) - Se separata ritningar för elektriska data","(3) - Se separata ritningar för elektriska data"]